VERSION 6		// V1 expects map checkpoint rectangles
// V2 and above expect map checkpoint points
// V3 and above expect splash file stuff at the end
// V4 and above expect two sets of PIX and MAT and ped substitution entry
-143.7, 8, -122.6		// Position of centre of start of grid
360								// Direction that grid faces in
// Laps, checkpoints etc
180,90,30							// Initial timer count for each skill level
1									// # laps
5000,5000,5000						// Race completed bonus (all laps raced) for each skill level
10000,10000,10000					// Race completed bonus (all peds killed) for each skill level
10000,10000,10000					// Race completed bonus (all oppos wasted) for each skill level
// Width and height of map checkpoint rectangles
9,18
11,26
4									// # checkpoints
// Checkpoint #1
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-123.653,-100,-135.5					// Point #0
-123.653,100,-135.5						// Point #1
-125.46,100,-130.5						// Point #2
-125.46,-100,-130.5					// Point #3
22,22	//X,X(LO/HI)
55,55		//Y,Y(LO/HI)
// Checkpoint #2
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-96.4,-100,70.4						// Point #0
-96.4.762,100,70.4						// Point #1
-97.74,100,76.6						// Point #2
-97.74,-100,76.6					// Point #3
76,76
144,144
// Checkpoint #3
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
71.353,-100,38.31						// Point #0
71.353,100,38.31						// Point #1
76.06,100,39.5						// Point #2
76.06,-100,39.5					// Point #3
293,293	//X,X(LO/HI)
128,128		//Y,Y(LO/HI)
// Checkpoint #4
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
8.17,-100,-234.8						// Point #0
8.17,100,-234.8						// Point #1
4.86,100,-231.3						// Point #2
4.86,-100,-231.3					// Point #3
202,202	//X,X(LO/HI)
13,13		//Y,Y(LO/HI)
3									// # pixelmap files to load
NEWYORK.PIX
NEWYORKH.PIX
FOGSCRN.PIX
3									// # pixelmap files to load
NEWYORK.PIX
NEWYORKH.PIX
FOGSCRN.PIX
2									// # shade table files to load
IDENTITY.TAB
DRRENDER.TAB
5									// # material files to load
NEWYORK.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT
WATTY.MAT
5									// # material files to load
NEWYORK.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT
WATTY.MAT
1									// # model files to load
NEWYORK.DAT
1									// # model files to load
NEWYORK.DAT
NEWYORK.ACT                                                     // Track actor
NEWYORK.ACT                                                     // Track actor
DEFAULTX.ACT							// Additional actor
// HORIZON STUFF
NEWYORKH.PIX						// Name of sky texture pixelmap (or "none")
7									// Horizontal repetitions of sky texture
30									// Vertical size of sky texture (degrees)
150									// Position of horizon (pixels below top)
fog							// Depth cue mode ("none", "dark" or "fog")
5,0									// Degree of fog/darkness
// DEFAULT ENGINE NOISE
0
// SPECIAL EFFECTS VOLUMES
0				// # special effects volumes
// REFLECTIVE WINDSCREEN SPECIFICATIONS
FOGSCRN.MAT							// Material to use for default screens
DRKSCRN.MAT							// Material to use for default screens during darkness
FOGSCRN.MAT							// Material to use for default screens during fog
0									// (ignore) # areas with different screens
// MAP DETAILS
NEWY_MAP.PIX						// Map pixelmap name
1.315,	0.000,	0		// World->map transformation matrix
0,	0,	0
0,	0.419,	0
201.415, 117.403, 0.007
// ****** START OF FUNK AND GROOVE STUFF ******
START OF FUNK

END OF FUNK

START OF GROOVE

END OF GROOVE
// ****** START OF PEDESTRIAN STUFF ******

0				// Ped subs table index

940				// Number of pedestrians

// Pedestrian number 1

99				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-144.885,-0.582,-124.100
	point
	-144.134,-0.726,-127.800
	reverse


// Pedestrian number 2

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-134.138,-0.979,-137.065
	point
	-131.443,-1.176,-136.632
	reverse


// Pedestrian number 3

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-130.362,-1.069,-132.399
	point
	-128.309,-0.908,-131.979
	reverse


// Pedestrian number 4

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-129.763,-1.071,-136.114
	point
	-131.316,-1.161,-136.401
	reverse


// Pedestrian number 5

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-138.566,-0.591,-136.786
	point
	-140.170,-0.548,-136.068
	reverse


// Pedestrian number 6

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-142.803,-0.673,-133.232
	point
	-144.355,-0.777,-129.904
	reverse


// Pedestrian number 7

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-145.729,-0.650,-121.639
	point
	-145.696,-0.881,-118.917
	reverse


// Pedestrian number 8

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-145.656,-0.942,-116.996
	point
	-145.692,-0.871,-115.671
	reverse


// Pedestrian number 9

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-142.265,-0.914,-117.758
	point
	-142.285,-0.732,-119.986
	reverse


// Pedestrian number 10

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-141.354,-0.768,-128.088
	point
	-140.899,-0.838,-129.738
	reverse


// Pedestrian number 11

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-139.007,-0.831,-132.961
	point
	-138.173,-0.811,-133.428
	reverse


// Pedestrian number 12

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-135.071,-0.961,-133.243
	point
	-132.607,-1.162,-132.917
	reverse


// Pedestrian number 13

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-127.046,-0.870,-131.877
	point
	-123.630,-0.804,-131.163
	reverse


// Pedestrian number 14

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-114.697,-1.210,-127.285
	point
	-113.153,-1.173,-126.886
	reverse


// Pedestrian number 15

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-108.958,-1.448,-126.194
	point
	-107.030,-1.606,-126.147
	reverse


// Pedestrian number 16

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-105.261,-1.586,-129.655
	point
	-106.876,-1.536,-129.505
	reverse


// Pedestrian number 17

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-115.106,-1.284,-131.033
	point
	-117.578,-1.079,-132.172
	reverse


// Pedestrian number 18

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-121.866,-0.763,-134.249
	point
	-124.549,-0.841,-134.873
	reverse


// Pedestrian number 19

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-134.930,-0.893,-136.932
	point
	-136.418,-0.734,-137.016
	reverse


// Pedestrian number 20

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-141.371,-0.575,-135.076
	point
	-142.204,-0.622,-134.111
	reverse


// Pedestrian number 21

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-145.245,-0.630,-125.764
	point
	-145.455,-0.584,-124.415
	reverse


// Pedestrian number 22

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-142.485,-0.742,-119.924
	point
	-142.370,-0.642,-121.080
	reverse


// Pedestrian number 23

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-142.182,-0.578,-122.983
	point
	-141.804,-0.648,-125.615
	reverse


// Pedestrian number 24

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-140.293,-0.857,-131.453
	point
	-139.503,-0.856,-132.358
	reverse


// Pedestrian number 25

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-127.499,-0.899,-135.665
	point
	-126.323,-0.858,-135.353
	reverse


// Pedestrian number 26

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-118.712,-0.972,-129.157
	point
	-117.782,-1.089,-128.613
	reverse


// Pedestrian number 27

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-110.816,-1.211,-129.929
	point
	-112.272,-1.188,-130.288
	reverse


// Pedestrian number 28

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-120.222,-0.805,-129.993
	point
	-121.475,-0.753,-130.638
	reverse


// Pedestrian number 29

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-114.620,-1.280,-130.756
	point
	-113.490,-1.236,-130.530
	reverse


// Pedestrian number 30

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-109.390,-1.326,-129.553
	point
	-107.939,-1.461,-129.371
	reverse


// Pedestrian number 31

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-102.120,-1.485,-129.838
	point
	-99.982,-1.291,-129.625
	reverse


// Pedestrian number 32

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-97.978,-0.994,-125.685
	point
	-99.724,-1.214,-126.006
	reverse


// Pedestrian number 33

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-102.405,-1.531,-126.437
	point
	-104.143,-1.638,-126.410
	reverse


// Pedestrian number 34

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-110.891,-1.256,-126.508
	point
	-111.919,-1.191,-126.631
	reverse


// Pedestrian number 35

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-115.001,-1.217,-127.386
	point
	-116.163,-1.221,-127.798
	reverse


// Pedestrian number 36

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-119.742,-0.798,-133.413
	point
	-118.841,-0.892,-133.028
	reverse


// Pedestrian number 37

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-105.685,-1.650,-126.266
	point
	-104.869,-1.651,-126.350
	reverse


// Pedestrian number 38

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-101.311,-1.416,-126.414
	point
	-99.501,-1.187,-126.250
	reverse


// Pedestrian number 39

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-94.118,-0.901,-124.918
	point
	-92.117,-1.193,-124.275
	reverse


// Pedestrian number 40

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-89.903,-1.393,-123.501
	point
	-88.572,-1.333,-122.891
	reverse


// Pedestrian number 41

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-84.363,-1.199,-121.926
	point
	-80.873,-1.217,-122.418
	reverse


// Pedestrian number 42

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-78.677,-1.001,-122.834
	point
	-75.867,-0.692,-123.351
	reverse


// Pedestrian number 43

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-72.483,-0.512,-126.640
	point
	-73.456,-0.522,-126.768
	reverse


// Pedestrian number 44

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-75.755,-0.707,-126.628
	point
	-77.981,-0.984,-126.241
	reverse


// Pedestrian number 45

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-81.196,-1.251,-125.630
	point
	-83.591,-1.193,-125.275
	reverse


// Pedestrian number 46

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-86.459,-1.205,-125.679
	point
	-88.410,-1.362,-126.434
	reverse


// Pedestrian number 47

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-91.124,-1.269,-127.616
	point
	-93.251,-0.984,-128.198
	reverse


// Pedestrian number 48

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-98.282,-1.104,-129.210
	point
	-99.823,-1.266,-129.435
	reverse


// Pedestrian number 49

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-102.686,-1.510,-129.689
	point
	-104.692,-1.587,-129.691
	reverse


// Pedestrian number 50

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-105.758,-1.577,-129.532
	point
	-105.036,-1.583,-129.624
	reverse


// Pedestrian number 51

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-100.432,-1.327,-129.543
	point
	-98.935,-1.173,-129.348
	reverse


// Pedestrian number 52

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-95.679,-0.903,-128.706
	point
	-94.455,-0.899,-128.415
	reverse


// Pedestrian number 53

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-90.220,-1.359,-127.273
	point
	-89.276,-1.395,-126.925
	reverse


// Pedestrian number 54

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-84.382,-1.164,-125.232
	point
	-83.584,-1.189,-125.327
	reverse


// Pedestrian number 55

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-79.597,-1.157,-125.840
	point
	-77.867,-0.962,-126.118
	reverse


// Pedestrian number 56

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-78.943,-1.030,-122.862
	point
	-80.399,-1.177,-122.532
	reverse


// Pedestrian number 57

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-85.602,-1.167,-121.969
	point
	-87.272,-1.224,-122.398
	reverse


// Pedestrian number 58

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-91.534,-1.274,-124.184
	point
	-92.996,-1.043,-124.762
	reverse


// Pedestrian number 59

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-96.619,-0.865,-125.528
	point
	-95.431,-0.828,-125.255
	reverse


// Pedestrian number 60

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-70.741,-0.659,-125.885
	point
	-69.367,-0.872,-125.001
	reverse


// Pedestrian number 61

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-67.724,-1.056,-123.849
	point
	-66.105,-1.075,-122.903
	reverse


// Pedestrian number 62

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-64.342,-1.033,-122.275
	point
	-62.688,-1.066,-121.782
	reverse


// Pedestrian number 63

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-61.869,-1.109,-121.566
	point
	-60.996,-1.164,-121.668
	reverse


// Pedestrian number 64

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-60.228,-1.214,-121.547
	point
	-59.730,-1.252,-120.965
	reverse


// Pedestrian number 65

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-65.120,-1.041,-118.882
	point
	-66.439,-1.076,-119.401
	reverse


// Pedestrian number 66

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-68.164,-1.092,-120.300
	point
	-69.714,-0.973,-121.347
	reverse


// Pedestrian number 67

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-71.624,-0.712,-122.686
	point
	-72.482,-0.623,-123.195
	reverse


// Pedestrian number 68

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-73.510,-0.584,-123.427
	point
	-74.859,-0.620,-123.406
	reverse


// Pedestrian number 69

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-74.959,-0.613,-126.533
	point
	-74.465,-0.567,-126.565
	reverse


// Pedestrian number 70

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-73.564,-0.516,-126.612
	point
	-72.773,-0.501,-126.573
	reverse


// Pedestrian number 71

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-71.641,-0.551,-126.345
	point
	-71.035,-0.625,-126.089
	reverse


// Pedestrian number 72

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-69.615,-0.966,-121.656
	point
	-70.257,-0.879,-122.096
	reverse


// Pedestrian number 73

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-63.323,-1.078,-118.317
	point
	-62.242,-1.146,-117.862
	reverse


// Pedestrian number 74

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-60.666,-1.260,-116.969
	point
	-58.367,-1.337,-115.875
	reverse


// Pedestrian number 75

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-56.021,-1.261,-114.824
	point
	-53.636,-1.088,-114.054
	reverse


// Pedestrian number 76

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-50.413,-1.145,-113.121
	point
	-48.314,-1.420,-112.568
	reverse


// Pedestrian number 77

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-46.304,-1.637,-112.595
	point
	-45.862,-1.659,-112.783
	reverse


// Pedestrian number 78

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-46.293,-1.563,-116.091
	point
	-47.522,-1.391,-116.793
	reverse


// Pedestrian number 79

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-49.159,-1.181,-117.515
	point
	-50.590,-1.045,-117.736
	reverse


// Pedestrian number 80

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-52.076,-1.041,-117.996
	point
	-54.050,-1.162,-118.426
	reverse


// Pedestrian number 81

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-57.125,-1.324,-119.329
	point
	-60.403,-1.219,-120.873
	reverse


// Pedestrian number 82

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-59.716,-1.301,-117.243
	point
	-58.454,-1.332,-116.326
	reverse


// Pedestrian number 83

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-57.238,-1.320,-115.377
	point
	-56.498,-1.284,-114.816
	reverse


// Pedestrian number 84

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-55.184,-1.191,-114.045
	point
	-53.782,-1.091,-113.641
	reverse


// Pedestrian number 85

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-48.922,-1.326,-113.155
	point
	-47.555,-1.500,-113.053
	reverse


// Pedestrian number 86

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-45.739,-1.614,-116.163
	point
	-46.790,-1.485,-116.723
	reverse


// Pedestrian number 87

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-48.554,-1.258,-117.004
	point
	-49.446,-1.168,-116.841
	reverse


// Pedestrian number 88

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-52.261,-1.047,-117.641
	point
	-53.324,-1.103,-117.833
	reverse


// Pedestrian number 89

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-54.840,-1.178,-114.875
	point
	-53.891,-1.108,-114.607
	reverse


// Pedestrian number 90

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-50.425,-1.133,-113.671
	point
	-49.080,-1.298,-113.428
	reverse


// Pedestrian number 91

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-42.329,-1.269,-112.607
	point
	-41.119,-0.965,-112.655
	reverse


// Pedestrian number 92

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-37.360,-0.841,-112.735
	point
	-36.031,-1.120,-112.466
	reverse


// Pedestrian number 93

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-33.617,-1.412,-111.588
	point
	-31.397,-1.298,-110.909
	reverse


// Pedestrian number 94

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-29.686,-1.201,-110.497
	point
	-27.769,-1.165,-110.213
	reverse


// Pedestrian number 95

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-26.349,-1.162,-110.025
	point
	-25.056,-1.166,-109.849
	reverse


// Pedestrian number 96

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-25.537,-1.090,-113.419
	point
	-26.929,-1.140,-113.633
	reverse


// Pedestrian number 97

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-28.612,-1.189,-113.850
	point
	-30.257,-1.271,-114.105
	reverse


// Pedestrian number 98

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-33.417,-1.398,-114.946
	point
	-34.941,-1.200,-115.444
	reverse


// Pedestrian number 99

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-39.224,-0.744,-116.054
	point
	-40.545,-1.015,-115.971
	reverse


// Pedestrian number 100

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-43.234,-1.611,-115.780
	point
	-45.149,-1.669,-115.801
	reverse


// Pedestrian number 101

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-44.456,-1.652,-112.691
	point
	-43.698,-1.556,-112.506
	reverse


// Pedestrian number 102

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-35.185,-1.290,-112.049
	point
	-34.406,-1.379,-111.834
	reverse


// Pedestrian number 103

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-37.029,-0.769,-115.972
	point
	-37.675,-0.685,-116.062
	reverse


// Pedestrian number 104

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-42.978,-1.565,-115.605
	point
	-41.961,-1.365,-115.811
	reverse


// Pedestrian number 105

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-32.046,-1.391,-114.684
	point
	-30.918,-1.318,-114.247
	reverse


// Pedestrian number 106

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-27.827,-1.161,-113.489
	point
	-26.100,-1.113,-113.306
	reverse


// Pedestrian number 107

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-23.691,-0.976,-112.972
	point
	-22.071,-0.854,-112.571
	reverse


// Pedestrian number 108

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-19.686,-0.764,-111.435
	point
	-18.034,-0.738,-110.218
	reverse


// Pedestrian number 109

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-16.487,-0.725,-108.383
	point
	-15.818,-0.678,-106.931
	reverse


// Pedestrian number 110

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-15.091,-0.657,-104.727
	point
	-15.161,-0.669,-103.440
	reverse


// Pedestrian number 111

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-19.184,-1.436,-103.369
	point
	-19.197,-1.437,-104.844
	reverse


// Pedestrian number 112

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-20.619,-1.309,-108.197
	point
	-21.815,-1.233,-108.871
	reverse


// Pedestrian number 113

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-23.398,-1.181,-109.493
	point
	-25.499,-1.165,-110.032
	reverse


// Pedestrian number 114

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-28.516,-1.172,-110.599
	point
	-30.139,-1.219,-110.796
	reverse


// Pedestrian number 115

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-33.903,-1.349,-115.304
	point
	-32.611,-1.404,-114.891
	reverse


// Pedestrian number 116

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-29.322,-1.217,-113.856
	point
	-27.955,-1.166,-113.445
	reverse


// Pedestrian number 117

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-22.949,-0.932,-112.564
	point
	-21.178,-0.803,-112.149
	reverse


// Pedestrian number 118

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-16.566,-0.735,-108.013
	point
	-15.862,-0.712,-106.430
	reverse


// Pedestrian number 119

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-15.356,-0.686,-104.687
	point
	-15.590,-0.731,-103.295
	reverse


// Pedestrian number 120

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-19.207,-1.434,-105.377
	point
	-19.483,-1.410,-106.638
	reverse


// Pedestrian number 121

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-19.911,-1.367,-107.529
	point
	-20.549,-1.312,-108.173
	reverse


// Pedestrian number 122

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-18.779,-0.753,-110.641
	point
	-17.661,-0.737,-109.747
	reverse


// Pedestrian number 123

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-14.785,-0.643,-105.259
	point
	-14.596,-0.644,-104.068
	reverse


// Pedestrian number 124

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-14.776,-0.649,-102.379
	point
	-15.249,-0.675,-101.563
	reverse


// Pedestrian number 125

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-18.979,-1.430,-102.607
	point
	-19.411,-1.432,-100.874
	reverse


// Pedestrian number 126

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-15.494,-0.716,-100.513
	point
	-15.656,-0.774,-99.114
	reverse


// Pedestrian number 127

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-15.650,-0.812,-97.305
	point
	-15.535,-0.760,-95.636
	reverse


// Pedestrian number 128

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-15.761,-0.770,-94.315
	point
	-16.249,-0.806,-92.826
	reverse


// Pedestrian number 129

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-17.104,-0.799,-90.661
	point
	-17.776,-0.767,-89.343
	reverse


// Pedestrian number 130

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-20.212,-0.953,-87.642
	point
	-21.450,-1.017,-87.213
	reverse


// Pedestrian number 131

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-22.976,-1.032,-86.670
	point
	-24.228,-1.032,-86.249
	reverse


// Pedestrian number 132

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-25.703,-1.063,-85.866
	point
	-27.030,-1.127,-85.805
	reverse


// Pedestrian number 133

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-29.831,-1.296,-86.278
	point
	-31.308,-1.353,-86.657
	reverse


// Pedestrian number 134

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-29.773,-1.327,-89.591
	point
	-28.342,-1.260,-89.455
	reverse


// Pedestrian number 135

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-26.626,-1.172,-89.279
	point
	-25.296,-1.140,-89.241
	reverse


// Pedestrian number 136

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-23.905,-1.166,-89.454
	point
	-22.955,-1.210,-89.761
	reverse


// Pedestrian number 137

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-20.930,-1.357,-91.639
	point
	-20.799,-1.387,-92.275
	reverse


// Pedestrian number 138

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-20.313,-1.431,-94.462
	point
	-20.157,-1.435,-95.652
	reverse


// Pedestrian number 139

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-19.839,-1.438,-98.150
	point
	-19.652,-1.435,-99.524
	reverse


// Pedestrian number 140

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-19.275,-1.431,-101.534
	point
	-19.242,-1.429,-101.994
	reverse


// Pedestrian number 141

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-15.586,-0.726,-101.872
	point
	-15.606,-0.730,-101.167
	reverse


// Pedestrian number 142

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-15.995,-0.916,-96.798
	point
	-16.311,-0.980,-94.944
	reverse


// Pedestrian number 143

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-16.750,-0.986,-93.163
	point
	-17.111,-0.951,-91.800
	reverse


// Pedestrian number 144

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-18.557,-0.991,-89.461
	point
	-19.123,-0.953,-88.594
	reverse


// Pedestrian number 145

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-21.705,-0.899,-86.527
	point
	-22.930,-0.885,-85.862
	reverse


// Pedestrian number 146

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-25.056,-1.041,-85.981
	point
	-25.705,-1.073,-86.048
	reverse


// Pedestrian number 147

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-27.949,-1.190,-86.185
	point
	-29.048,-1.256,-86.252
	reverse


// Pedestrian number 148

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-33.353,-1.350,-87.031
	point
	-35.236,-1.331,-87.153
	reverse


// Pedestrian number 149

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-37.090,-1.348,-87.030
	point
	-38.040,-1.363,-86.832
	reverse


// Pedestrian number 150

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-39.265,-1.318,-86.177
	point
	-39.941,-1.329,-85.589
	reverse


// Pedestrian number 151

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-41.029,-1.327,-84.132
	point
	-42.206,-1.334,-81.888
	reverse


// Pedestrian number 152

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-43.559,-1.434,-78.592
	point
	-44.378,-1.445,-76.209
	reverse


// Pedestrian number 153

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-45.384,-1.152,-73.178
	point
	-46.020,-0.810,-71.483
	reverse


// Pedestrian number 154

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-47.070,-0.471,-68.487
	point
	-47.324,-0.590,-67.294
	reverse


// Pedestrian number 155

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-47.949,-0.942,-64.896
	point
	-48.885,-0.973,-62.526
	reverse


// Pedestrian number 156

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-50.451,-0.799,-60.446
	point
	-51.815,-0.674,-58.973
	reverse


// Pedestrian number 157

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-53.628,-0.571,-57.295
	point
	-55.468,-0.586,-55.983
	reverse


// Pedestrian number 158

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-59.130,-0.818,-55.143
	point
	-60.787,-0.920,-55.350
	reverse


// Pedestrian number 159

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-64.058,-0.894,-57.090
	point
	-65.447,-0.903,-57.703
	reverse


// Pedestrian number 160

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-62.924,-0.917,-60.417
	point
	-62.188,-0.939,-60.175
	reverse


// Pedestrian number 161

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-61.019,-0.990,-59.690
	point
	-60.199,-1.028,-59.316
	reverse


// Pedestrian number 162

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-58.398,-1.073,-58.809
	point
	-57.591,-1.052,-58.688
	reverse


// Pedestrian number 163

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-56.680,-1.038,-59.065
	point
	-56.076,-1.022,-59.433
	reverse


// Pedestrian number 164

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-54.377,-0.923,-60.800
	point
	-53.609,-0.916,-61.931
	reverse


// Pedestrian number 165

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-52.659,-0.982,-63.894
	point
	-52.278,-0.956,-65.620
	reverse


// Pedestrian number 166

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-51.639,-0.638,-67.976
	point
	-50.869,-0.462,-69.482
	reverse


// Pedestrian number 167

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-49.591,-0.711,-71.967
	point
	-49.175,-0.937,-73.058
	reverse


// Pedestrian number 168

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-48.313,-1.311,-75.330
	point
	-47.383,-1.451,-77.785
	reverse


// Pedestrian number 169

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-46.292,-1.382,-80.661
	point
	-46.071,-1.361,-81.242
	reverse


// Pedestrian number 170

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-44.326,-1.300,-84.951
	point
	-43.581,-1.277,-86.175
	reverse


// Pedestrian number 171

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-41.995,-1.231,-87.840
	point
	-40.814,-1.234,-88.897
	reverse


// Pedestrian number 172

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-38.402,-1.226,-90.067
	point
	-36.720,-1.244,-90.414
	reverse


// Pedestrian number 173

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-34.048,-1.311,-90.439
	point
	-32.108,-1.354,-90.253
	reverse


// Pedestrian number 174

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-30.429,-1.352,-89.908
	point
	-29.027,-1.300,-89.615
	reverse


// Pedestrian number 175

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-26.663,-1.167,-89.149
	point
	-25.675,-1.140,-89.048
	reverse


// Pedestrian number 176

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-23.329,-0.954,-86.074
	point
	-24.050,-0.952,-85.712
	reverse


// Pedestrian number 177

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-30.619,-1.352,-89.726
	point
	-31.377,-1.356,-89.990
	reverse


// Pedestrian number 178

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-34.586,-1.296,-90.338
	point
	-36.133,-1.259,-90.373
	reverse


// Pedestrian number 179

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-38.916,-1.227,-89.710
	point
	-40.115,-1.226,-89.214
	reverse


// Pedestrian number 180

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-42.531,-1.255,-87.089
	point
	-43.084,-1.270,-86.484
	reverse


// Pedestrian number 181

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-45.978,-1.376,-80.695
	point
	-46.530,-1.412,-79.707
	reverse


// Pedestrian number 182

6				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	-47.258,-1.445,-78.235
	point
	-47.331,-1.446,-78.013
	point
	-48.108,-1.319,-75.372
	reverse


// Pedestrian number 183

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-48.491,-1.171,-74.274
	point
	-48.901,-1.061,-73.677
	reverse


// Pedestrian number 184

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-50.120,-0.501,-70.674
	point
	-50.360,-0.451,-69.968
	reverse


// Pedestrian number 185

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-51.608,-0.821,-66.737
	point
	-52.161,-0.981,-65.114
	reverse


// Pedestrian number 186

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-53.171,-0.945,-62.823
	point
	-53.425,-0.931,-62.402
	reverse


// Pedestrian number 187

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-54.992,-0.958,-60.307
	point
	-55.339,-0.982,-59.975
	reverse


// Pedestrian number 188

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-64.741,-0.940,-61.453
	point
	-66.458,-0.945,-61.970
	reverse


// Pedestrian number 189

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-69.224,-0.694,-62.536
	point
	-70.647,-0.516,-62.744
	reverse


// Pedestrian number 190

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-76.838,-0.569,-63.009
	point
	-78.102,-0.724,-63.127
	reverse


// Pedestrian number 191

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-79.749,-0.852,-63.325
	point
	-80.958,-0.873,-63.469
	reverse


// Pedestrian number 192

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-81.207,-0.923,-59.967
	point
	-80.300,-0.844,-59.867
	reverse


// Pedestrian number 193

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-78.595,-0.616,-59.685
	point
	-77.139,-0.426,-59.531
	reverse


// Pedestrian number 194

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-74.762,-0.314,-59.400
	point
	-73.006,-0.390,-59.415
	reverse


// Pedestrian number 195

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-70.461,-0.681,-59.055
	point
	-69.115,-0.840,-58.722
	reverse


// Pedestrian number 196

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-63.262,-0.914,-56.751
	point
	-62.685,-0.930,-55.928
	reverse


// Pedestrian number 197

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-61.713,-0.935,-55.257
	point
	-60.479,-0.895,-54.874
	reverse


// Pedestrian number 198

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-58.139,-0.749,-55.526
	point
	-57.367,-0.691,-55.746
	reverse


// Pedestrian number 199

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-56.277,-0.617,-56.079
	point
	-55.466,-0.580,-56.381
	reverse


// Pedestrian number 200

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-53.006,-0.603,-58.099
	point
	-51.960,-0.670,-59.065
	reverse


// Pedestrian number 201

22				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	-50.291,-0.861,-61.290
	point
	-50.052,-0.894,-61.679
	point
	-48.984,-1.000,-63.987
	reverse


// Pedestrian number 202

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-47.950,-0.734,-66.465
	point
	-47.468,-0.533,-67.831
	reverse


// Pedestrian number 203

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-46.916,-0.514,-69.796
	point
	-46.348,-0.786,-71.456
	reverse


// Pedestrian number 204

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-45.767,-1.092,-72.942
	point
	-45.027,-1.351,-74.772
	reverse


// Pedestrian number 205

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-43.748,-1.456,-77.711
	point
	-43.102,-1.413,-79.177
	reverse


// Pedestrian number 206

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-42.270,-1.340,-81.601
	point
	-42.026,-1.325,-82.551
	reverse


// Pedestrian number 207

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-44.605,-1.406,-75.452
	point
	-44.870,-1.329,-74.518
	reverse


// Pedestrian number 208

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-49.313,-0.944,-62.152
	point
	-49.802,-0.847,-60.858
	reverse


// Pedestrian number 209

4				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	-51.544,-0.671,-58.780
	point
	-51.843,-0.648,-58.431
	point
	-53.252,-0.578,-57.142
	reverse


// Pedestrian number 210

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-60.348,-0.908,-55.849
	point
	-61.437,-0.942,-56.009
	reverse


// Pedestrian number 211

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-81.664,-0.856,-63.097
	point
	-82.514,-0.825,-63.110
	reverse


// Pedestrian number 212

1				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	-84.160,-0.740,-62.838
	point
	-84.371,-0.727,-62.713
	point
	-85.301,-0.667,-62.176
	reverse


// Pedestrian number 213

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-86.761,-0.560,-60.869
	point
	-87.262,-0.518,-60.266
	reverse


// Pedestrian number 214

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-91.746,-0.657,-54.796
	point
	-92.347,-0.668,-53.305
	reverse


// Pedestrian number 215

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-93.085,-0.385,-50.427
	point
	-93.165,-0.320,-49.709
	reverse


// Pedestrian number 216

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-93.528,-0.248,-48.679
	point
	-93.950,-0.221,-47.655
	reverse


// Pedestrian number 217

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-90.345,-0.248,-47.414
	point
	-90.017,-0.288,-48.249
	reverse


// Pedestrian number 218

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-88.278,-0.691,-53.326
	point
	-87.732,-0.638,-54.293
	reverse


// Pedestrian number 219

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-86.563,-0.502,-56.588
	point
	-85.865,-0.550,-57.449
	reverse


// Pedestrian number 220

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-83.002,-0.923,-59.578
	point
	-82.031,-0.947,-59.869
	reverse


// Pedestrian number 221

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-81.731,-0.854,-63.466
	point
	-82.096,-0.840,-63.492
	reverse


// Pedestrian number 222

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-84.395,-0.717,-62.201
	point
	-85.318,-0.653,-61.625
	reverse


// Pedestrian number 223

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-87.864,-0.508,-60.471
	point
	-88.757,-0.462,-59.523
	reverse


// Pedestrian number 224

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-90.764,-0.585,-55.665
	point
	-91.597,-0.686,-53.706
	reverse


// Pedestrian number 225

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-92.635,-0.514,-51.526
	point
	-93.407,-0.420,-50.840
	reverse


// Pedestrian number 226

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-93.647,-0.336,-50.070
	point
	-93.631,-0.285,-49.394
	reverse


// Pedestrian number 227

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-87.731,-0.602,-54.824
	point
	-87.031,-0.520,-55.915
	reverse


// Pedestrian number 228

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-103.788,-0.307,-4.601
	point
	-103.648,-0.287,-3.427
	reverse


// Pedestrian number 229

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-102.950,-0.337,-1.561
	point
	-102.091,-0.396,-0.268
	reverse


// Pedestrian number 230

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-100.564,-0.541,1.146
	point
	-99.773,-0.597,1.717
	reverse


// Pedestrian number 231

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-98.894,-0.929,-2.076
	point
	-99.602,-0.801,-2.776
	reverse


// Pedestrian number 232

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-100.607,-0.738,-5.799
	point
	-100.497,-0.773,-6.983
	reverse


// Pedestrian number 233

6				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	-100.215,-0.770,-7.817
	point
	-100.110,-0.765,-8.022
	point
	-99.590,-0.714,-9.403
	reverse


// Pedestrian number 234

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-98.772,-0.486,-14.956
	point
	-98.794,-0.466,-15.861
	reverse


// Pedestrian number 235

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-98.757,-0.461,-16.924
	point
	-98.703,-0.470,-17.760
	reverse


// Pedestrian number 236

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-101.863,-0.700,-18.241
	point
	-101.984,-0.691,-17.694
	reverse


// Pedestrian number 237

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-102.121,-0.662,-16.380
	point
	-102.210,-0.647,-15.767
	reverse


// Pedestrian number 238

25				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	-102.562,-0.665,-14.602
	point
	-102.630,-0.659,-14.263
	point
	-102.649,-0.643,-13.772
	reverse


// Pedestrian number 239

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-103.521,-0.320,-3.319
	point
	-103.385,-0.302,-2.568
	reverse


// Pedestrian number 240

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-101.841,-0.494,-0.444
	point
	-101.143,-0.524,0.456
	reverse


// Pedestrian number 241

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-99.933,-0.731,-3.360
	point
	-100.365,-0.688,-4.620
	reverse


// Pedestrian number 242

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-90.074,-0.718,0.849
	point
	-89.524,-0.663,0.865
	reverse


// Pedestrian number 243

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-89.216,-0.595,2.065
	point
	-89.437,-0.600,2.925
	reverse


// Pedestrian number 244

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-89.567,-0.601,3.432
	point
	-89.688,-0.602,3.905
	reverse


// Pedestrian number 245

7				// Ref num
4				// Number of instructions
3				// Initial instruction

	point
	-90.245,-0.644,4.563
	point
	-91.154,-0.737,4.472
	point
	-91.573,-0.773,4.403
	reverse


// Pedestrian number 246

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-94.446,-0.851,3.721
	point
	-95.578,-0.832,3.397
	reverse


// Pedestrian number 247

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-95.415,-0.977,-0.486
	point
	-94.316,-0.923,-0.364
	reverse


// Pedestrian number 248

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-92.774,-0.871,-0.001
	point
	-91.697,-0.835,0.312
	reverse


// Pedestrian number 249

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-89.435,-0.616,2.274
	point
	-89.898,-0.628,3.793
	reverse


// Pedestrian number 250

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-89.866,-0.605,4.437
	point
	-89.333,-0.537,4.800
	reverse


// Pedestrian number 251

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-85.869,-0.291,5.653
	point
	-85.152,-0.304,5.965
	reverse


// Pedestrian number 252

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-83.945,-0.372,6.310
	point
	-82.929,-0.469,6.546
	reverse


// Pedestrian number 253

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-82.472,-0.417,2.857
	point
	-82.960,-0.371,2.577
	reverse


// Pedestrian number 254

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-83.690,-0.318,2.330
	point
	-84.017,-0.305,2.258
	reverse


// Pedestrian number 255

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-84.675,-0.292,2.941
	point
	-84.861,-0.291,3.428
	reverse


// Pedestrian number 256

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-85.162,-0.292,4.120
	point
	-85.300,-0.289,4.650
	reverse


// Pedestrian number 257

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-85.237,-0.294,5.109
	point
	-85.175,-0.294,5.218
	reverse


// Pedestrian number 258

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-85.002,-0.291,4.024
	point
	-84.899,-0.290,2.926
	reverse


// Pedestrian number 259

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-80.874,-0.603,3.224
	point
	-79.048,-0.785,3.587
	reverse


// Pedestrian number 260

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-76.879,-0.852,4.150
	point
	-75.239,-0.806,4.862
	reverse


// Pedestrian number 261

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-73.675,-0.724,5.868
	point
	-72.657,-0.669,6.906
	reverse


// Pedestrian number 262

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-71.388,-0.652,8.377
	point
	-70.879,-0.671,9.316
	reverse


// Pedestrian number 263

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-70.665,-0.722,10.941
	point
	-70.655,-0.783,12.307
	reverse


// Pedestrian number 264

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-70.583,-0.913,14.855
	point
	-70.504,-0.973,16.438
	reverse


// Pedestrian number 265

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-70.550,-0.942,17.643
	point
	-70.836,-1.003,20.057
	reverse


// Pedestrian number 266

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-71.489,-0.973,23.007
	point
	-71.959,-0.896,25.035
	reverse


// Pedestrian number 267

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-73.593,-0.530,30.912
	point
	-74.068,-0.551,32.549
	reverse


// Pedestrian number 268

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-74.820,-0.655,35.082
	point
	-75.484,-0.652,36.989
	reverse


// Pedestrian number 269

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-76.134,-0.600,38.497
	point
	-76.801,-0.569,39.546
	reverse


// Pedestrian number 270

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-78.237,-0.558,40.953
	point
	-80.092,-0.614,42.092
	reverse


// Pedestrian number 271

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-82.270,-0.662,42.968
	point
	-84.038,-0.621,43.000
	reverse


// Pedestrian number 272

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-86.975,-0.551,42.307
	point
	-87.596,-0.571,42.182
	reverse


// Pedestrian number 273

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-88.841,-0.639,41.931
	point
	-89.771,-0.691,41.769
	reverse


// Pedestrian number 274

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-88.103,-0.563,38.155
	point
	-87.136,-0.620,38.233
	reverse


// Pedestrian number 275

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-85.689,-0.704,38.582
	point
	-83.994,-0.754,39.029
	reverse


// Pedestrian number 276

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-82.363,-0.754,39.198
	point
	-81.412,-0.722,39.073
	reverse


// Pedestrian number 277

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-80.437,-0.675,38.608
	point
	-79.789,-0.649,38.060
	reverse


// Pedestrian number 278

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-79.022,-0.663,36.780
	point
	-78.591,-0.692,35.546
	reverse


// Pedestrian number 279

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-78.194,-0.676,33.976
	point
	-77.730,-0.574,31.931
	reverse


// Pedestrian number 280

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-76.701,-0.672,27.236
	point
	-76.147,-0.853,24.718
	reverse


// Pedestrian number 281

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-75.518,-0.977,21.866
	point
	-74.773,-1.005,18.485
	reverse


// Pedestrian number 282

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-73.844,-0.929,13.915
	point
	-73.793,-0.894,12.949
	reverse


// Pedestrian number 283

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-74.110,-0.863,11.005
	point
	-74.681,-0.859,9.743
	reverse


// Pedestrian number 284

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-76.245,-0.869,8.463
	point
	-78.320,-0.862,7.708
	reverse


// Pedestrian number 285

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-80.672,-0.734,7.115
	point
	-81.874,-0.598,6.824
	reverse


// Pedestrian number 286

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-78.868,-0.796,3.787
	point
	-77.968,-0.834,3.823
	reverse


// Pedestrian number 287

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-75.053,-0.792,5.208
	point
	-74.205,-0.748,5.634
	reverse


// Pedestrian number 288

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-71.422,-0.662,9.160
	point
	-71.148,-0.680,9.794
	reverse


// Pedestrian number 289

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-70.382,-0.817,12.952
	point
	-70.149,-0.866,14.022
	reverse


// Pedestrian number 290

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-71.205,-0.986,18.481
	point
	-71.398,-0.997,19.358
	reverse


// Pedestrian number 291

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-71.815,-0.999,21.377
	point
	-72.170,-0.964,23.126
	reverse


// Pedestrian number 292

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-73.010,-0.797,26.513
	point
	-73.398,-0.675,28.124
	reverse


// Pedestrian number 293

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-74.046,-0.526,31.104
	point
	-74.429,-0.572,32.943
	reverse


// Pedestrian number 294

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-75.374,-0.663,36.132
	point
	-75.967,-0.627,37.637
	reverse


// Pedestrian number 295

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-80.239,-0.621,42.161
	point
	-81.400,-0.653,42.859
	reverse


// Pedestrian number 296

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-83.704,-0.635,43.318
	point
	-84.781,-0.593,43.221
	reverse


// Pedestrian number 297

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-82.124,-0.656,43.326
	point
	-81.113,-0.642,43.169
	reverse


// Pedestrian number 298

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-79.534,-0.599,42.555
	point
	-78.402,-0.567,41.905
	reverse


// Pedestrian number 299

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-74.489,-0.646,34.824
	point
	-73.965,-0.593,33.590
	reverse


// Pedestrian number 300

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-72.952,-0.599,29.336
	point
	-72.660,-0.745,27.345
	reverse


// Pedestrian number 301

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-71.911,-0.955,23.543
	point
	-71.407,-1.005,21.223
	reverse


// Pedestrian number 302

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-70.930,-0.992,18.794
	point
	-70.759,-0.958,16.479
	reverse


// Pedestrian number 303

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-77.449,-0.870,7.673
	point
	-78.857,-0.845,7.339
	reverse


// Pedestrian number 304

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-81.293,-0.661,6.730
	point
	-82.689,-0.495,6.379
	reverse


// Pedestrian number 305

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-75.343,-0.858,8.713
	point
	-74.695,-0.847,9.370
	reverse


// Pedestrian number 306

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-74.058,-0.979,15.520
	point
	-74.359,-0.970,17.328
	reverse


// Pedestrian number 307

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-74.915,-1.007,19.828
	point
	-75.351,-0.978,21.828
	reverse


// Pedestrian number 308

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-76.020,-0.838,25.026
	point
	-76.379,-0.710,26.842
	reverse


// Pedestrian number 309

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-76.718,-0.589,28.473
	point
	-76.929,-0.544,29.393
	reverse


// Pedestrian number 310

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-77.921,-0.660,33.714
	point
	-78.363,-0.682,35.646
	reverse


// Pedestrian number 311

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-91.021,-0.465,38.104
	point
	-92.198,-0.472,38.212
	reverse


// Pedestrian number 312

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-94.170,-0.552,39.208
	point
	-95.677,-0.670,40.592
	reverse


// Pedestrian number 313

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-96.840,-0.796,42.693
	point
	-97.350,-0.859,44.461
	reverse


// Pedestrian number 314

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-98.126,-0.848,47.005
	point
	-98.681,-0.786,49.258
	reverse


// Pedestrian number 315

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-99.336,-0.606,52.645
	point
	-99.580,-0.411,53.911
	reverse


// Pedestrian number 316

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-99.437,-0.049,56.245
	point
	-98.937,-0.020,56.660
	reverse


// Pedestrian number 317

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-98.273,-0.024,56.808
	point
	-97.681,-0.030,56.916
	reverse


// Pedestrian number 318

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-96.645,-0.232,55.693
	point
	-96.340,-0.435,54.602
	reverse


// Pedestrian number 319

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-95.738,-0.717,52.183
	point
	-95.200,-0.794,49.760
	reverse


// Pedestrian number 320

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-94.655,-0.873,47.306
	point
	-94.230,-0.899,45.420
	reverse


// Pedestrian number 321

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-93.533,-0.856,43.725
	point
	-93.033,-0.813,42.929
	reverse


// Pedestrian number 322

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-89.748,-0.684,41.643
	point
	-89.025,-0.640,41.635
	reverse


// Pedestrian number 323

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-94.784,-0.871,47.209
	point
	-95.212,-0.817,48.846
	reverse


// Pedestrian number 324

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-98.723,-0.624,61.663
	point
	-99.660,-0.636,61.533
	reverse


// Pedestrian number 325

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-100.116,-0.637,61.465
	point
	-100.564,-0.641,61.436
	reverse


// Pedestrian number 326

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-101.217,-0.693,61.918
	point
	-101.529,-0.713,63.265
	reverse


// Pedestrian number 327

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-101.859,-0.574,65.445
	point
	-101.832,-0.479,67.358
	reverse


// Pedestrian number 328

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-101.339,-0.427,70.130
	point
	-100.539,-0.379,72.132
	reverse


// Pedestrian number 329

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-98.731,-0.270,74.376
	point
	-97.028,-0.249,75.474
	reverse


// Pedestrian number 330

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-93.386,-0.403,76.118
	point
	-91.417,-0.541,76.238
	reverse


// Pedestrian number 331

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-88.546,-0.721,76.052
	point
	-87.127,-0.795,75.990
	reverse


// Pedestrian number 332

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-85.507,-0.830,72.496
	point
	-86.431,-0.784,72.354
	reverse


// Pedestrian number 333

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-88.104,-0.696,72.344
	point
	-89.676,-0.617,72.457
	reverse


// Pedestrian number 334

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-91.480,-0.553,72.584
	point
	-92.514,-0.543,72.585
	reverse


// Pedestrian number 335

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-93.937,-0.559,72.411
	point
	-95.462,-0.618,72.017
	reverse


// Pedestrian number 336

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-96.483,-0.677,71.514
	point
	-97.396,-0.720,70.823
	reverse


// Pedestrian number 337

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-98.641,-0.796,66.089
	point
	-98.355,-0.838,64.723
	reverse


// Pedestrian number 338

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-98.065,-0.800,63.254
	point
	-97.938,-0.734,62.589
	reverse


// Pedestrian number 339

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-98.855,-0.658,61.847
	point
	-99.574,-0.695,61.922
	reverse


// Pedestrian number 340

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-101.571,-0.694,63.838
	point
	-101.778,-0.636,64.539
	reverse


// Pedestrian number 341

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-100.244,-0.381,72.404
	point
	-99.562,-0.320,73.477
	reverse


// Pedestrian number 342

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-96.148,-0.249,75.533
	point
	-95.027,-0.286,76.016
	reverse


// Pedestrian number 343

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-91.149,-0.558,76.064
	point
	-89.607,-0.655,75.965
	reverse


// Pedestrian number 344

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-76.897,-0.974,76.268
	point
	-76.231,-0.965,76.473
	reverse


// Pedestrian number 345

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-74.676,-0.941,77.255
	point
	-73.256,-0.928,77.831
	reverse


// Pedestrian number 346

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-70.145,-0.933,80.483
	point
	-69.861,-0.938,80.855
	reverse


// Pedestrian number 347

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-68.463,-0.957,83.738
	point
	-68.229,-0.965,84.588
	reverse


// Pedestrian number 348

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-67.933,-1.031,86.952
	point
	-68.110,-1.146,89.181
	reverse


// Pedestrian number 349

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-68.641,-1.197,92.259
	point
	-68.995,-1.133,93.807
	reverse


// Pedestrian number 350

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-73.521,-1.065,93.656
	point
	-73.252,-1.111,92.392
	reverse


// Pedestrian number 351

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-72.792,-1.177,90.381
	point
	-72.287,-1.106,88.148
	reverse


// Pedestrian number 352

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-71.874,-0.943,85.239
	point
	-72.265,-0.922,84.092
	reverse


// Pedestrian number 353

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-73.156,-0.914,82.362
	point
	-74.150,-0.918,81.493
	reverse


// Pedestrian number 354

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-75.739,-0.942,80.683
	point
	-77.089,-0.965,80.199
	reverse


// Pedestrian number 355

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-80.188,-0.990,78.788
	point
	-82.367,-0.966,77.494
	reverse


// Pedestrian number 356

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-83.639,-0.908,73.000
	point
	-82.435,-0.944,73.439
	reverse


// Pedestrian number 357

4				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-80.475,-0.981,74.423
	point
	-78.577,-0.992,75.500
	point
	-73.338,-0.930,77.046
	point
	-71.940,-0.926,77.830
	reverse


// Pedestrian number 358

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-69.244,-0.944,81.618
	point
	-68.723,-0.950,82.677
	reverse


// Pedestrian number 359

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-68.974,-1.191,92.257
	point
	-69.217,-1.131,93.674
	reverse


// Pedestrian number 360

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-70.338,-1.211,99.191
	point
	-70.339,-1.186,100.782
	reverse


// Pedestrian number 361

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-70.282,-1.105,102.219
	point
	-70.579,-0.995,103.298
	reverse


// Pedestrian number 362

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-71.477,-0.704,106.123
	point
	-70.553,-0.748,106.712
	reverse


// Pedestrian number 363

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-68.712,-0.922,107.745
	point
	-66.682,-0.991,108.654
	reverse


// Pedestrian number 364

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-63.115,-0.823,109.823
	point
	-61.006,-0.634,110.403
	reverse


// Pedestrian number 365

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-58.754,-0.537,111.057
	point
	-58.131,-0.541,111.456
	reverse


// Pedestrian number 366

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-56.731,-0.602,113.144
	point
	-56.666,-0.595,113.826
	reverse


// Pedestrian number 367

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-56.729,-0.591,114.659
	point
	-56.843,-0.590,115.710
	reverse


// Pedestrian number 368

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-56.940,-0.587,116.245
	point
	-57.409,-0.596,117.070
	reverse


// Pedestrian number 369

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-59.125,-0.543,116.237
	point
	-59.972,-0.534,115.620
	reverse


// Pedestrian number 370

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-61.641,-0.607,114.631
	point
	-63.077,-0.731,114.126
	reverse


// Pedestrian number 371

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-65.588,-0.937,113.370
	point
	-67.575,-0.986,112.909
	reverse


// Pedestrian number 372

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-69.724,-0.898,112.402
	point
	-71.371,-0.741,111.564
	reverse


// Pedestrian number 373

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-72.903,-0.544,109.875
	point
	-73.985,-0.460,108.557
	reverse


// Pedestrian number 374

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-75.252,-0.538,106.607
	point
	-75.550,-0.638,105.363
	reverse


// Pedestrian number 375

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-75.807,-0.912,102.605
	point
	-75.169,-1.153,99.577
	reverse


// Pedestrian number 376

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-73.915,-1.109,96.323
	point
	-73.652,-1.059,94.759
	reverse


// Pedestrian number 377

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-73.027,-1.124,92.205
	point
	-72.331,-1.164,89.420
	reverse


// Pedestrian number 378

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-72.035,-1.080,87.769
	point
	-71.928,-1.004,86.589
	reverse


// Pedestrian number 379

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-75.020,-1.023,101.604
	point
	-75.224,-0.913,102.670
	reverse


// Pedestrian number 380

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-75.206,-0.740,104.307
	point
	-74.945,-0.581,105.971
	reverse


// Pedestrian number 381

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-69.584,-0.900,112.088
	point
	-68.352,-0.966,112.670
	reverse


// Pedestrian number 382

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-66.999,-0.980,113.388
	point
	-65.558,-0.927,113.818
	reverse


// Pedestrian number 383

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-63.598,-0.774,114.306
	point
	-62.082,-0.637,114.832
	reverse


// Pedestrian number 384

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-60.478,-0.543,115.266
	point
	-59.708,-0.535,115.454
	reverse


// Pedestrian number 385

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-61.516,-0.680,109.841
	point
	-62.949,-0.815,109.283
	reverse


// Pedestrian number 386

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-67.418,-0.984,108.735
	point
	-68.891,-0.916,108.238
	reverse


// Pedestrian number 387

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-34.858,-1.228,114.945
	point
	-33.817,-1.300,114.921
	reverse


// Pedestrian number 388

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-32.009,-1.392,114.906
	point
	-30.823,-1.443,114.904
	reverse


// Pedestrian number 389

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-28.448,-1.619,114.883
	point
	-26.389,-1.826,114.958
	reverse


// Pedestrian number 390

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-23.478,-1.987,115.294
	point
	-21.659,-2.074,115.108
	reverse


// Pedestrian number 391

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-18.544,-2.459,114.881
	point
	-17.318,-2.561,115.096
	reverse


// Pedestrian number 392

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-14.362,-2.220,116.434
	point
	-13.561,-2.001,117.486
	reverse


// Pedestrian number 393

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-11.780,-1.605,119.865
	point
	-9.882,-1.468,121.600
	reverse


// Pedestrian number 394

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-5.563,-1.603,123.748
	point
	-4.296,-1.713,124.323
	reverse


// Pedestrian number 395

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-0.053,-2.458,124.228
	point
	1.472,-2.680,123.992
	reverse


// Pedestrian number 396

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	4.182,-2.640,124.433
	point
	5.652,-2.284,125.345
	reverse


// Pedestrian number 397

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	11.033,-1.414,128.120
	point
	12.244,-1.444,128.733
	reverse


// Pedestrian number 398

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	15.312,-1.531,129.878
	point
	16.519,-1.520,130.024
	reverse


// Pedestrian number 399

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	16.336,-1.373,126.817
	point
	15.583,-1.425,126.247
	reverse


// Pedestrian number 400

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	14.196,-1.519,125.471
	point
	13.287,-1.564,125.299
	reverse


// Pedestrian number 401

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	12.026,-1.635,124.866
	point
	10.835,-1.738,124.119
	reverse


// Pedestrian number 402

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	8.185,-2.192,122.527
	point
	6.565,-2.540,121.822
	reverse


// Pedestrian number 403

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	3.908,-2.914,120.711
	point
	2.171,-2.915,120.649
	reverse


// Pedestrian number 404

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-2.543,-2.240,121.646
	point
	-3.323,-2.152,121.301
	reverse


// Pedestrian number 405

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-5.612,-1.916,120.121
	point
	-6.819,-1.816,119.467
	reverse


// Pedestrian number 406

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-13.254,-1.924,114.002
	point
	-13.888,-2.041,113.298
	reverse


// Pedestrian number 407

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-15.457,-2.167,111.687
	point
	-16.410,-2.108,111.186
	reverse


// Pedestrian number 408

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-23.312,-1.637,111.421
	point
	-24.457,-1.694,111.579
	reverse


// Pedestrian number 409

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-28.349,-1.467,111.685
	point
	-28.799,-1.398,111.678
	reverse


// Pedestrian number 410

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-32.193,-0.979,111.581
	point
	-33.127,-0.942,111.646
	reverse


// Pedestrian number 411

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-36.402,-1.070,112.818
	point
	-37.047,-1.129,113.166
	reverse


// Pedestrian number 412

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-34.937,-0.978,112.002
	point
	-34.344,-0.955,111.710
	reverse


// Pedestrian number 413

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-27.636,-1.517,112.047
	point
	-26.256,-1.638,112.141
	reverse


// Pedestrian number 414

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-23.409,-1.673,111.920
	point
	-22.082,-1.649,111.798
	reverse


// Pedestrian number 415

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-15.358,-2.222,112.045
	point
	-14.534,-2.107,112.382
	reverse


// Pedestrian number 416

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-11.440,-1.621,115.477
	point
	-10.681,-1.600,116.594
	reverse


// Pedestrian number 417

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-1.729,-2.449,121.093
	point
	-0.581,-2.606,121.189
	reverse


// Pedestrian number 418

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	4.906,-2.824,121.036
	point
	5.837,-2.701,121.123
	reverse


// Pedestrian number 419

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	13.634,-1.544,125.835
	point
	15.002,-1.460,126.461
	reverse


// Pedestrian number 420

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	15.169,-1.506,129.476
	point
	14.425,-1.508,129.429
	reverse


// Pedestrian number 421

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	7.937,-1.808,126.043
	point
	6.525,-2.156,125.244
	reverse


// Pedestrian number 422

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	3.473,-2.739,123.888
	point
	1.869,-2.714,123.692
	reverse


// Pedestrian number 423

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-1.528,-2.187,124.263
	point
	-2.801,-1.937,124.734
	reverse


// Pedestrian number 424

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-6.424,-1.440,124.099
	point
	-7.870,-1.419,123.193
	reverse


// Pedestrian number 425

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-10.315,-1.504,121.005
	point
	-11.356,-1.581,119.887
	reverse


// Pedestrian number 426

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-18.487,-2.437,114.194
	point
	-19.829,-2.253,114.218
	reverse


// Pedestrian number 427

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-23.163,-1.955,114.836
	point
	-24.603,-1.918,114.996
	reverse


// Pedestrian number 428

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-27.432,-1.794,115.210
	point
	-29.609,-1.589,115.144
	reverse


// Pedestrian number 429

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-36.686,-1.212,115.396
	point
	-38.021,-1.281,116.040
	reverse


// Pedestrian number 430

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-38.934,-2.005,123.983
	point
	-40.602,-2.183,124.024
	reverse


// Pedestrian number 431

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-45.895,-2.504,123.399
	point
	-47.870,-2.334,122.830
	reverse


// Pedestrian number 432

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-52.444,-1.178,118.153
	point
	-51.918,-1.243,118.193
	reverse


// Pedestrian number 433

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-46.739,-2.381,119.776
	point
	-44.912,-2.513,120.304
	reverse


// Pedestrian number 434

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-40.473,-2.255,120.915
	point
	-38.771,-2.065,120.995
	reverse


// Pedestrian number 435

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-28.596,-2.385,122.210
	point
	-26.386,-2.534,122.421
	reverse


// Pedestrian number 436

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-10.102,-2.563,130.399
	point
	-8.601,-2.573,131.210
	reverse


// Pedestrian number 437

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-3.300,-3.177,131.055
	point
	-1.819,-3.446,130.670
	reverse


// Pedestrian number 438

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	10.052,-2.432,134.940
	point
	10.829,-2.374,135.357
	reverse


// Pedestrian number 439

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	13.756,-2.279,136.221
	point
	15.371,-2.280,136.270
	reverse


// Pedestrian number 440

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	20.993,-2.486,136.690
	point
	23.543,-2.536,137.454
	reverse


// Pedestrian number 441

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	27.036,-2.160,138.570
	point
	28.248,-1.866,138.960
	reverse


// Pedestrian number 442

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	28.416,-1.640,142.379
	point
	27.081,-1.975,141.958
	reverse


// Pedestrian number 443

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	23.997,-2.488,140.987
	point
	21.910,-2.537,140.332
	reverse


// Pedestrian number 444

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	17.270,-2.349,139.027
	point
	15.456,-2.291,138.892
	reverse


// Pedestrian number 445

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	9.561,-2.418,137.987
	point
	8.590,-2.515,137.235
	reverse


// Pedestrian number 446

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	3.737,-3.460,134.430
	point
	1.889,-3.715,133.881
	reverse


// Pedestrian number 447

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-3.294,-3.333,133.852
	point
	-4.894,-3.024,134.186
	reverse


// Pedestrian number 448

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-11.994,-2.563,132.403
	point
	-13.217,-2.596,131.288
	reverse


// Pedestrian number 449

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-18.258,-3.335,127.257
	point
	-19.488,-3.391,126.776
	reverse


// Pedestrian number 450

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-23.218,-2.890,126.244
	point
	-24.655,-2.692,126.028
	reverse


// Pedestrian number 451

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-33.467,-1.945,124.864
	point
	-34.780,-1.869,124.703
	reverse


// Pedestrian number 452

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-45.839,-2.476,120.402
	point
	-47.392,-2.304,119.812
	reverse


// Pedestrian number 453

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-49.879,-1.699,118.984
	point
	-50.908,-1.354,118.665
	reverse


// Pedestrian number 454

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-52.155,-1.446,121.441
	point
	-50.972,-1.718,121.882
	reverse


// Pedestrian number 455

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-45.013,-2.522,123.380
	point
	-42.867,-2.424,123.766
	reverse


// Pedestrian number 456

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-19.821,-3.321,123.549
	point
	-18.645,-3.391,123.692
	reverse


// Pedestrian number 457

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	-15.855,-3.059,125.181
	point
	-14.608,-2.818,126.182
	reverse


// Pedestrian number 458

17				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	3.030,-3.670,131.224
	point
	4.151,-3.506,131.380
	reverse


// Pedestrian number 459

12				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	6.239,-3.072,132.167
	point
	6.990,-2.909,132.548
	reverse


// Pedestrian number 460

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	39.959,-1.014,147.311
	point
	39.399,-1.014,147.111
	reverse


// Pedestrian number 461

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	35.456,-1.047,144.869
	point
	34.812,-1.054,144.418
	reverse


// Pedestrian number 462

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	33.893,-1.061,143.384
	point
	34.009,-1.061,142.606
	reverse


// Pedestrian number 463

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	34.282,-1.063,141.543
	point
	34.579,-1.064,140.171
	reverse


// Pedestrian number 464

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	34.718,-1.062,139.420
	point
	34.792,-1.063,138.985
	reverse


// Pedestrian number 465

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	34.478,-1.063,139.781
	point
	33.814,-1.067,142.537
	reverse


// Pedestrian number 466

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	35.844,-1.043,144.871
	point
	36.878,-1.030,145.408
	reverse


// Pedestrian number 467

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	37.998,-1.018,145.906
	point
	39.179,-1.016,146.350
	reverse


// Pedestrian number 468

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	40.498,-1.014,143.077
	point
	39.822,-1.018,142.411
	reverse


// Pedestrian number 469

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	38.906,-1.018,141.619
	point
	38.120,-1.026,141.089
	reverse


// Pedestrian number 470

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	36.973,-1.041,140.414
	point
	36.257,-1.048,140.330
	reverse


// Pedestrian number 471

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	37.835,-1.026,141.395
	point
	38.555,-1.022,142.018
	reverse


// Pedestrian number 472

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	39.358,-1.014,142.577
	point
	39.852,-1.014,142.902
	reverse


// Pedestrian number 473

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	44.104,-0.981,147.881
	point
	44.853,-0.946,148.271
	reverse


// Pedestrian number 474

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	45.748,-0.901,148.557
	point
	46.710,-0.860,148.439
	reverse


// Pedestrian number 475

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	48.309,-0.812,148.207
	point
	49.492,-0.806,148.005
	reverse


// Pedestrian number 476

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	52.663,-0.887,147.441
	point
	54.262,-0.943,147.114
	reverse


// Pedestrian number 477

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	58.875,-1.045,146.397
	point
	60.448,-1.056,146.515
	reverse


// Pedestrian number 478

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	62.704,-1.043,146.923
	point
	64.052,-0.984,147.515
	reverse


// Pedestrian number 479

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.651,-0.741,148.279
	point
	67.777,-0.621,148.410
	reverse


// Pedestrian number 480

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	70.366,-0.419,148.562
	point
	71.680,-0.374,148.449
	reverse


// Pedestrian number 481

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	75.114,-0.390,147.268
	point
	75.880,-0.424,146.566
	reverse


// Pedestrian number 482

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	72.011,-1.035,144.841
	point
	71.268,-1.054,144.587
	reverse


// Pedestrian number 483

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	70.533,-1.061,144.380
	point
	69.860,-1.058,144.406
	reverse


// Pedestrian number 484

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.554,-1.056,144.520
	point
	67.674,-1.049,144.504
	reverse


// Pedestrian number 485

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.078,-1.057,144.056
	point
	64.955,-1.062,143.673
	reverse


// Pedestrian number 486

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	63.045,-1.064,142.924
	point
	61.940,-1.058,142.540
	reverse


// Pedestrian number 487

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	59.318,-1.034,142.219
	point
	57.661,-1.007,142.528
	reverse


// Pedestrian number 488

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	54.527,-0.918,143.428
	point
	53.155,-0.871,143.879
	reverse


// Pedestrian number 489

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	50.868,-0.813,144.421
	point
	49.889,-0.807,144.552
	reverse


// Pedestrian number 490

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	47.191,-0.878,144.638
	point
	45.391,-0.963,144.442
	reverse


// Pedestrian number 491

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	43.027,-1.024,143.969
	point
	41.694,-1.020,143.637
	reverse


// Pedestrian number 492

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	41.247,-1.020,147.414
	point
	42.059,-1.020,147.883
	reverse


// Pedestrian number 493

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	43.202,-1.005,148.305
	point
	43.855,-0.984,148.328
	reverse


// Pedestrian number 494

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	46.249,-0.884,148.189
	point
	46.657,-0.866,148.162
	reverse


// Pedestrian number 495

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	53.305,-0.912,147.611
	point
	54.332,-0.946,147.407
	reverse


// Pedestrian number 496

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	56.681,-1.008,146.737
	point
	58.341,-1.037,146.099
	reverse


// Pedestrian number 497

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.544,-1.058,146.097
	point
	62.313,-1.053,146.402
	reverse


// Pedestrian number 498

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	63.473,-1.019,146.920
	point
	64.933,-0.929,147.552
	reverse


// Pedestrian number 499

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.684,-0.570,148.203
	point
	70.393,-0.457,148.252
	reverse


// Pedestrian number 500

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	72.596,-0.392,148.078
	point
	74.296,-0.338,147.968
	reverse


// Pedestrian number 501

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	76.325,-0.557,145.235
	point
	76.950,-0.604,144.400
	reverse


// Pedestrian number 502

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	78.409,-0.846,141.496
	point
	78.975,-0.998,140.116
	reverse


// Pedestrian number 503

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	79.417,-1.169,138.616
	point
	79.922,-1.316,136.583
	reverse


// Pedestrian number 504

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	75.246,-1.290,137.431
	point
	74.663,-1.245,138.260
	reverse


// Pedestrian number 505

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	74.137,-1.181,139.382
	point
	73.867,-1.116,140.744
	reverse


// Pedestrian number 506

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	73.608,-1.080,142.025
	point
	73.254,-1.063,142.993
	reverse


// Pedestrian number 507

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.952,-1.043,144.788
	point
	68.134,-1.042,144.734
	reverse


// Pedestrian number 508

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	64.722,-1.062,143.699
	point
	63.434,-1.062,143.144
	reverse


// Pedestrian number 509

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	56.880,-0.991,142.980
	point
	55.431,-0.948,143.252
	reverse


// Pedestrian number 510

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	48.726,-0.821,144.785
	point
	47.855,-0.848,144.646
	reverse


// Pedestrian number 511

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	45.238,-0.970,144.220
	point
	43.690,-1.012,143.997
	reverse


// Pedestrian number 512

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	40.874,-1.020,147.790
	point
	41.498,-1.018,147.920
	reverse


// Pedestrian number 513

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	72.052,-1.061,144.342
	point
	72.723,-1.057,143.966
	reverse


// Pedestrian number 514

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	73.682,-1.056,142.957
	point
	73.971,-1.067,142.357
	reverse


// Pedestrian number 515

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	74.527,-1.133,140.468
	point
	74.646,-1.166,139.795
	reverse


// Pedestrian number 516

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	75.323,-1.353,134.821
	point
	75.519,-1.339,133.407
	reverse


// Pedestrian number 517

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	75.926,-1.247,131.084
	point
	76.185,-1.176,129.779
	reverse


// Pedestrian number 518

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	75.799,-0.930,125.572
	point
	75.212,-0.815,124.891
	reverse


// Pedestrian number 519

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	74.594,-0.728,124.236
	point
	74.488,-0.715,124.113
	reverse


// Pedestrian number 520

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	76.475,-0.996,120.981
	point
	77.324,-1.028,121.463
	reverse


// Pedestrian number 521

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	79.091,-1.055,123.024
	point
	79.880,-1.061,124.069
	reverse


// Pedestrian number 522

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	80.874,-1.074,126.596
	point
	81.069,-1.089,127.772
	reverse


// Pedestrian number 523

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	80.736,-1.281,132.533
	point
	80.494,-1.323,133.694
	reverse


// Pedestrian number 524

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	79.961,-1.340,135.680
	point
	79.655,-1.308,136.737
	reverse


// Pedestrian number 525

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	79.227,-1.190,138.411
	point
	78.919,-1.065,139.612
	reverse


// Pedestrian number 526

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	78.029,-0.801,142.028
	point
	77.593,-0.707,143.090
	reverse


// Pedestrian number 527

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	74.031,-0.394,147.630
	point
	73.439,-0.401,147.763
	reverse


// Pedestrian number 528

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	69.339,-1.038,144.873
	point
	69.037,-1.063,144.174
	reverse


// Pedestrian number 529

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	75.782,-1.352,135.135
	point
	76.011,-1.345,134.115
	reverse


// Pedestrian number 530

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	76.323,-1.305,132.487
	point
	76.562,-1.242,131.058
	reverse


// Pedestrian number 531

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	76.696,-1.158,129.505
	point
	76.676,-1.094,128.145
	reverse


// Pedestrian number 532

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	76.466,-1.008,126.038
	point
	76.016,-0.908,125.147
	reverse


// Pedestrian number 533

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	72.502,-0.630,122.996
	point
	71.181,-0.620,122.817
	reverse


// Pedestrian number 534

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.670,-0.622,122.473
	point
	66.262,-0.634,121.943
	reverse


// Pedestrian number 535

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	60.204,-0.811,117.768
	point
	59.708,-0.846,117.040
	reverse


// Pedestrian number 536

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	58.860,-0.931,114.913
	point
	58.508,-0.966,113.797
	reverse


// Pedestrian number 537

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	58.291,-0.997,111.140
	point
	58.451,-0.980,109.677
	reverse


// Pedestrian number 538

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	58.681,-0.965,108.792
	point
	59.055,-0.967,107.578
	reverse


// Pedestrian number 539

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.146,-0.667,102.035
	point
	61.848,-0.267,100.266
	reverse


// Pedestrian number 540

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	62.385,-0.335,92.667
	point
	62.169,-0.852,90.884
	reverse


// Pedestrian number 541

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.236,-1.549,86.029
	point
	60.918,-1.543,83.570
	reverse


// Pedestrian number 542

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.601,-1.306,79.108
	point
	62.161,-1.253,77.186
	reverse


// Pedestrian number 543

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	63.533,-1.164,73.586
	point
	64.331,-1.074,71.312
	reverse


// Pedestrian number 544

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.023,-1.078,66.004
	point
	66.604,-1.143,63.583
	reverse


// Pedestrian number 545

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	67.240,-1.255,58.068
	point
	67.486,-1.264,55.748
	reverse


// Pedestrian number 546

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	67.940,-1.265,51.645
	point
	68.425,-1.267,49.568
	reverse


// Pedestrian number 547

10				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	69.920,-1.243,46.412
	point
	70.153,-1.222,45.346
	point
	70.291,-1.225,44.759
	reverse


// Pedestrian number 548

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	70.638,-1.222,43.214
	point
	71.033,-1.222,41.343
	reverse


// Pedestrian number 549

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	74.984,-1.208,42.947
	point
	74.790,-1.208,43.748
	reverse


// Pedestrian number 550

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	73.893,-1.249,47.035
	point
	73.709,-1.270,48.267
	reverse


// Pedestrian number 551

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	73.707,-1.265,50.023
	point
	73.692,-1.265,51.108
	reverse


// Pedestrian number 552

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	73.107,-1.265,53.178
	point
	72.617,-1.262,54.260
	reverse


// Pedestrian number 553

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	71.932,-1.259,57.453
	point
	72.046,-1.253,58.364
	reverse


// Pedestrian number 554

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	72.300,-1.231,60.466
	point
	72.288,-1.201,62.132
	reverse


// Pedestrian number 555

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	71.619,-1.113,65.498
	point
	70.962,-1.066,67.304
	reverse


// Pedestrian number 556

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	70.154,-1.036,69.350
	point
	69.300,-1.055,71.505
	reverse


// Pedestrian number 557

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	67.697,-1.217,76.197
	point
	67.166,-1.258,78.399
	reverse


// Pedestrian number 558

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.126,-1.509,83.700
	point
	65.868,-1.567,85.805
	reverse


// Pedestrian number 559

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	65.940,-1.287,89.551
	point
	66.169,-0.862,91.573
	reverse


// Pedestrian number 560

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.661,0.371,97.423
	point
	66.644,0.268,98.568
	reverse


// Pedestrian number 561

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.627,-0.074,100.316
	point
	66.610,-0.454,101.938
	reverse


// Pedestrian number 562

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.135,-0.935,104.801
	point
	65.480,-0.991,106.476
	reverse


// Pedestrian number 563

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	64.373,-0.973,108.410
	point
	63.730,-0.969,109.506
	reverse


// Pedestrian number 564

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	62.944,-0.998,111.044
	point
	62.827,-1.026,112.180
	reverse


// Pedestrian number 565

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	63.413,-1.058,114.036
	point
	63.508,-1.060,115.198
	reverse


// Pedestrian number 566

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	64.114,-1.030,116.806
	point
	65.078,-1.026,117.353
	reverse


// Pedestrian number 567

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	67.394,-0.908,118.440
	point
	68.464,-0.837,118.708
	reverse


// Pedestrian number 568

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	70.802,-0.759,119.109
	point
	72.245,-0.792,119.337
	reverse


// Pedestrian number 569

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	74.293,-0.901,119.897
	point
	75.619,-0.971,120.433
	reverse


// Pedestrian number 570

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	79.940,-1.061,124.334
	point
	80.366,-1.064,125.069
	reverse


// Pedestrian number 571

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	81.103,-1.110,128.770
	point
	80.985,-1.191,130.821
	reverse


// Pedestrian number 572

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	73.246,-0.645,123.440
	point
	72.241,-0.628,123.321
	reverse


// Pedestrian number 573

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	67.616,-0.622,122.131
	point
	66.653,-0.629,121.851
	reverse


// Pedestrian number 574

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	64.642,-0.655,121.218
	point
	63.010,-0.696,120.352
	reverse


// Pedestrian number 575

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.621,-0.743,119.319
	point
	60.884,-0.783,118.338
	reverse


// Pedestrian number 576

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	60.022,-0.843,116.967
	point
	59.513,-0.884,116.082
	reverse


// Pedestrian number 577

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	58.656,-0.974,113.439
	point
	58.194,-0.996,112.108
	reverse


// Pedestrian number 578

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	57.879,-0.995,110.710
	point
	58.058,-0.982,109.670
	reverse


// Pedestrian number 579

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	60.196,-0.981,106.266
	point
	60.241,-0.986,105.418
	reverse


// Pedestrian number 580

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.117,-0.539,101.355
	point
	61.237,-0.338,100.471
	reverse


// Pedestrian number 581

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.624,-0.096,99.519
	point
	61.960,0.096,98.714
	reverse


// Pedestrian number 582

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	62.360,0.295,97.567
	point
	62.140,0.370,96.523
	reverse


// Pedestrian number 583

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.800,0.313,95.358
	point
	62.167,0.159,94.494
	reverse


// Pedestrian number 584

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.738,-0.526,91.922
	point
	61.421,-0.723,91.195
	reverse


// Pedestrian number 585

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.440,-1.121,89.621
	point
	61.518,-1.354,88.269
	reverse


// Pedestrian number 586

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.601,-1.538,86.198
	point
	61.608,-1.562,84.635
	reverse


// Pedestrian number 587

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.605,-1.489,82.501
	point
	61.668,-1.428,81.469
	reverse


// Pedestrian number 588

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	62.198,-1.319,79.538
	point
	62.574,-1.264,77.930
	reverse


// Pedestrian number 589

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	62.987,-1.220,75.608
	point
	63.020,-1.188,74.395
	reverse


// Pedestrian number 590

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	63.405,-1.119,72.518
	point
	64.122,-1.061,70.891
	reverse


// Pedestrian number 591

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	64.986,-1.033,68.949
	point
	65.855,-1.050,67.379
	reverse


// Pedestrian number 592

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.595,-1.084,65.744
	point
	66.858,-1.132,63.826
	reverse


// Pedestrian number 593

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	67.104,-1.203,61.171
	point
	66.987,-1.230,59.543
	reverse


// Pedestrian number 594

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.959,-1.253,57.620
	point
	67.127,-1.261,55.939
	reverse


// Pedestrian number 595

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	67.764,-1.263,53.758
	point
	68.435,-1.264,52.360
	reverse


// Pedestrian number 596

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.993,-1.266,50.664
	point
	69.038,-1.266,49.111
	reverse


// Pedestrian number 597

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	69.619,-1.264,49.219
	point
	68.843,-1.266,49.752
	reverse


// Pedestrian number 598

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.522,-1.261,50.487
	point
	68.566,-1.264,52.160
	reverse


// Pedestrian number 599

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.021,-1.260,54.655
	point
	67.785,-1.258,56.133
	reverse


// Pedestrian number 600

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	67.748,-1.250,57.902
	point
	67.689,-1.230,59.744
	reverse


// Pedestrian number 601

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	67.459,-1.194,61.646
	point
	67.163,-1.139,63.649
	reverse


// Pedestrian number 602

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.862,-1.090,65.601
	point
	66.607,-1.065,66.653
	reverse


// Pedestrian number 603

3				// Ref num
4				// Number of instructions
3				// Initial instruction

	point
	65.970,-1.037,68.697
	point
	65.333,-1.046,70.323
	point
	65.099,-1.061,70.920
	reverse


// Pedestrian number 604

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	63.573,-1.200,74.807
	point
	62.978,-1.233,76.337
	reverse


// Pedestrian number 605

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	62.059,-1.291,78.754
	point
	61.632,-1.344,80.032
	reverse


// Pedestrian number 606

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	65.596,-1.528,84.175
	point
	65.694,-1.502,83.613
	reverse


// Pedestrian number 607

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	65.990,-1.421,82.135
	point
	66.306,-1.374,81.435
	reverse


// Pedestrian number 608

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.827,-1.315,80.375
	point
	66.889,-1.273,79.046
	reverse


// Pedestrian number 609

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.722,-1.251,77.976
	point
	66.735,-1.234,77.162
	reverse


// Pedestrian number 610

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	67.512,-1.189,75.295
	point
	67.994,-1.172,74.823
	reverse


// Pedestrian number 611

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.774,-1.135,73.888
	point
	68.804,-1.102,73.059
	reverse


// Pedestrian number 612

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.680,-1.079,72.303
	point
	69.612,-1.053,71.591
	reverse


// Pedestrian number 613

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	70.241,-1.038,70.727
	point
	70.610,-1.034,69.642
	reverse


// Pedestrian number 614

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	70.907,-1.096,65.897
	point
	71.161,-1.137,64.433
	reverse


// Pedestrian number 615

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	71.590,-1.218,61.009
	point
	71.545,-1.243,59.342
	reverse


// Pedestrian number 616

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	72.003,-1.263,55.790
	point
	72.292,-1.263,54.139
	reverse


// Pedestrian number 617

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	72.856,-1.267,51.390
	point
	73.349,-1.267,49.432
	reverse


// Pedestrian number 618

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	73.998,-1.225,46.024
	point
	74.296,-1.238,44.681
	reverse


// Pedestrian number 619

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	74.729,-1.240,42.828
	point
	75.096,-1.241,41.260
	reverse


// Pedestrian number 620

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	70.874,-1.251,43.292
	point
	70.698,-1.250,44.099
	reverse


// Pedestrian number 621

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	69.648,-1.268,47.862
	point
	68.944,-1.263,48.706
	reverse


// Pedestrian number 622

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.390,-1.262,54.441
	point
	68.054,-1.259,56.348
	reverse


// Pedestrian number 623

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.490,-1.488,87.931
	point
	66.580,-1.234,89.969
	reverse


// Pedestrian number 624

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.719,-0.468,92.999
	point
	66.719,-0.097,94.269
	reverse


// Pedestrian number 625

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.783,-1.010,90.187
	point
	61.724,-1.326,88.518
	reverse


// Pedestrian number 626

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	64.591,-1.072,71.340
	point
	65.001,-1.037,69.529
	reverse


// Pedestrian number 627

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	73.450,-1.267,50.564
	point
	73.376,-1.264,52.024
	reverse


// Pedestrian number 628

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	73.119,-1.264,54.986
	point
	72.654,-1.262,56.413
	reverse


// Pedestrian number 629

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	70.358,-1.069,67.090
	point
	69.878,-1.037,69.319
	reverse


// Pedestrian number 630

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	65.497,-0.895,104.366
	point
	64.480,-0.989,106.150
	reverse


// Pedestrian number 631

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	63.495,-0.969,108.200
	point
	62.833,-0.974,109.752
	reverse


// Pedestrian number 632

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	72.261,-1.245,35.407
	point
	72.015,-1.225,34.467
	reverse


// Pedestrian number 633

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	71.661,-1.221,31.707
	point
	71.558,-1.228,30.394
	reverse


// Pedestrian number 634

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	71.375,-1.226,28.268
	point
	71.080,-1.216,26.016
	reverse


// Pedestrian number 635

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	72.103,-1.293,23.913
	point
	72.900,-1.292,23.480
	reverse


// Pedestrian number 636

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	73.453,-1.291,23.353
	point
	73.884,-1.289,23.251
	reverse


// Pedestrian number 637

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	75.012,-1.257,25.216
	point
	75.224,-1.243,26.079
	reverse


// Pedestrian number 638

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	75.636,-1.225,28.389
	point
	75.743,-1.224,29.438
	reverse


// Pedestrian number 639

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	75.946,-1.223,31.548
	point
	76.003,-1.222,32.148
	reverse


// Pedestrian number 640

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	75.701,-1.238,30.824
	point
	75.445,-1.248,28.967
	reverse


// Pedestrian number 641

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	73.238,-1.290,23.651
	point
	72.696,-1.292,23.855
	reverse


// Pedestrian number 642

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	71.415,-1.261,26.073
	point
	71.569,-1.267,27.199
	reverse


// Pedestrian number 643

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	71.863,-1.262,30.274
	point
	71.980,-1.251,32.038
	reverse


// Pedestrian number 644

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	70.487,-1.308,18.206
	point
	71.088,-1.307,17.583
	reverse


// Pedestrian number 645

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	71.740,-1.304,17.498
	point
	72.263,-1.303,17.581
	reverse


// Pedestrian number 646

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	71.017,-1.260,13.176
	point
	70.439,-1.270,12.481
	reverse


// Pedestrian number 647

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.979,-1.238,10.945
	point
	67.839,-1.196,9.862
	reverse


// Pedestrian number 648

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	65.558,-1.179,7.682
	point
	64.247,-1.163,6.467
	reverse


// Pedestrian number 649

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.879,-1.135,4.324
	point
	60.421,-1.121,3.050
	reverse


// Pedestrian number 650

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	58.735,-1.099,1.561
	point
	58.011,-1.089,0.873
	reverse


// Pedestrian number 651

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	56.816,-1.069,-0.829
	point
	56.562,-1.064,-1.565
	reverse


// Pedestrian number 652

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	56.065,-1.044,-4.738
	point
	56.024,-1.039,-6.178
	reverse


// Pedestrian number 653

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	54.835,-1.069,-8.697
	point
	54.337,-1.067,-8.723
	reverse


// Pedestrian number 654

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	53.673,-1.062,-8.794
	point
	53.208,-1.059,-8.851
	reverse


// Pedestrian number 655

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	52.174,-1.031,-6.809
	point
	52.094,-1.019,-5.989
	reverse


// Pedestrian number 656

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	52.280,-1.028,-4.009
	point
	52.497,-1.036,-2.720
	reverse


// Pedestrian number 657

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	52.942,-1.049,-0.680
	point
	53.419,-1.065,0.574
	reverse


// Pedestrian number 658

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	56.444,-1.106,4.216
	point
	57.677,-1.116,5.492
	reverse


// Pedestrian number 659

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	60.102,-1.138,7.988
	point
	61.443,-1.153,9.349
	reverse


// Pedestrian number 660

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	66.609,-1.273,15.068
	point
	67.459,-1.267,16.229
	reverse


// Pedestrian number 661

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	68.190,-1.252,17.322
	point
	68.691,-1.249,17.987
	reverse


// Pedestrian number 662

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	70.010,-1.308,18.067
	point
	72.054,-1.304,17.003
	reverse


// Pedestrian number 663

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	67.215,-1.208,9.437
	point
	66.148,-1.202,8.465
	reverse


// Pedestrian number 664

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	59.721,-1.138,7.465
	point
	58.847,-1.115,6.817
	reverse


// Pedestrian number 665

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	55.541,-1.084,3.455
	point
	54.893,-1.075,2.773
	reverse


// Pedestrian number 666

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	52.081,-1.011,-8.067
	point
	52.069,-1.012,-8.711
	reverse


// Pedestrian number 667

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	55.798,-1.055,-13.142
	point
	55.248,-1.050,-13.475
	reverse


// Pedestrian number 668

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	54.664,-1.045,-13.639
	point
	54.048,-1.040,-13.822
	reverse


// Pedestrian number 669

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	52.838,-0.976,-15.641
	point
	52.886,-0.967,-16.517
	reverse


// Pedestrian number 670

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	53.088,-0.957,-18.295
	point
	53.368,-0.947,-19.614
	reverse


// Pedestrian number 671

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	54.333,-0.945,-22.354
	point
	54.898,-0.950,-23.518
	reverse


// Pedestrian number 672

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	56.106,-0.949,-25.972
	point
	57.077,-0.953,-27.751
	reverse


// Pedestrian number 673

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	58.333,-0.943,-29.928
	point
	58.832,-0.945,-30.797
	reverse


// Pedestrian number 674

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	62.180,-0.979,-28.998
	point
	61.713,-0.985,-28.128
	reverse


// Pedestrian number 675

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	60.959,-0.988,-26.447
	point
	60.410,-0.988,-25.201
	reverse


// Pedestrian number 676

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	59.390,-0.991,-22.881
	point
	58.665,-0.993,-21.232
	reverse


// Pedestrian number 677

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	57.811,-0.990,-19.149
	point
	57.411,-0.994,-18.029
	reverse


// Pedestrian number 678

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	56.916,-1.005,-16.141
	point
	56.651,-1.013,-14.573
	reverse


// Pedestrian number 679

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	53.147,-0.976,-17.493
	point
	53.421,-0.984,-18.432
	reverse


// Pedestrian number 680

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	53.859,-0.967,-20.333
	point
	54.191,-0.964,-21.313
	reverse


// Pedestrian number 681

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	54.990,-0.966,-23.297
	point
	55.874,-0.969,-25.059
	reverse


// Pedestrian number 682

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	57.377,-0.970,-27.894
	point
	58.223,-0.961,-29.398
	reverse


// Pedestrian number 683

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	63.074,-0.913,-37.688
	point
	62.698,-0.936,-38.912
	reverse


// Pedestrian number 684

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	61.532,-0.914,-41.723
	point
	60.828,-0.903,-43.092
	reverse


// Pedestrian number 685

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	59.626,-0.885,-45.209
	point
	58.807,-0.872,-46.392
	reverse


// Pedestrian number 686

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	58.106,-0.864,-47.323
	point
	57.687,-0.859,-47.861
	reverse


// Pedestrian number 687

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	56.324,-0.896,-48.174
	point
	55.697,-0.893,-47.960
	reverse


// Pedestrian number 688

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	55.128,-0.891,-47.581
	point
	54.698,-0.890,-47.215
	reverse


// Pedestrian number 689

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	54.724,-0.855,-45.684
	point
	55.059,-0.854,-45.159
	reverse


// Pedestrian number 690

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	55.787,-0.862,-44.088
	point
	56.435,-0.874,-43.136
	reverse


// Pedestrian number 691

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	57.972,-0.908,-40.580
	point
	58.323,-0.906,-39.677
	reverse


// Pedestrian number 692

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	59.264,-0.920,-36.893
	point
	59.568,-0.930,-35.201
	reverse


// Pedestrian number 693

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	63.420,-0.974,-33.548
	point
	63.516,-0.963,-34.414
	reverse


// Pedestrian number 694

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	62.731,-0.948,-38.443
	point
	62.472,-0.942,-39.227
	reverse


// Pedestrian number 695

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	60.348,-0.912,-43.638
	point
	59.617,-0.905,-44.849
	reverse


// Pedestrian number 696

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	58.548,-0.887,-46.496
	point
	58.136,-0.881,-47.042
	reverse


// Pedestrian number 697

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	59.770,-0.951,-33.798
	point
	59.818,-0.953,-34.563
	reverse


// Pedestrian number 698

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	58.983,-0.932,-38.505
	point
	58.621,-0.923,-39.324
	reverse


// Pedestrian number 699

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	57.167,-0.911,-42.411
	point
	56.535,-0.903,-43.517
	reverse


// Pedestrian number 700

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	50.968,-0.847,-50.820
	point
	51.055,-0.846,-51.153
	reverse


// Pedestrian number 701

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	51.482,-0.847,-51.569
	point
	51.899,-0.848,-51.991
	reverse


// Pedestrian number 702

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	51.252,-0.803,-54.327
	point
	50.567,-0.783,-54.953
	reverse


// Pedestrian number 703

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	48.140,-0.754,-56.522
	point
	46.753,-0.742,-57.357
	reverse


// Pedestrian number 704

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	42.759,-0.706,-59.674
	point
	40.761,-0.686,-60.659
	reverse


// Pedestrian number 705

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	36.713,-0.655,-58.396
	point
	37.437,-0.662,-57.883
	reverse


// Pedestrian number 706

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	39.791,-0.676,-56.362
	point
	41.226,-0.690,-55.518
	reverse


// Pedestrian number 707

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	43.660,-0.714,-53.964
	point
	45.294,-0.728,-52.818
	reverse


// Pedestrian number 708

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	47.315,-0.747,-51.403
	point
	47.646,-0.750,-51.179
	reverse


// Pedestrian number 709

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	48.485,-0.755,-50.832
	point
	48.937,-0.769,-51.166
	reverse


// Pedestrian number 710

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	48.432,-0.789,-52.036
	point
	47.854,-0.768,-52.196
	reverse


// Pedestrian number 711

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	46.285,-0.744,-52.878
	point
	45.153,-0.732,-53.488
	reverse


// Pedestrian number 712

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	42.949,-0.714,-54.938
	point
	41.775,-0.709,-55.731
	reverse


// Pedestrian number 713

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	39.335,-0.703,-57.158
	point
	38.076,-0.694,-57.867
	reverse


// Pedestrian number 714

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	36.431,-0.666,-58.807
	point
	35.694,-0.651,-59.271
	reverse


// Pedestrian number 715

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	41.056,-0.707,-60.311
	point
	42.382,-0.716,-59.698
	reverse


// Pedestrian number 716

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	44.946,-0.743,-58.272
	point
	46.261,-0.753,-57.488
	reverse


// Pedestrian number 717

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	47.991,-0.769,-56.431
	point
	49.275,-0.783,-55.646
	reverse


// Pedestrian number 718

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	45.821,-0.766,-53.555
	point
	44.923,-0.757,-54.088
	reverse


// Pedestrian number 719

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	42.229,-0.730,-55.689
	point
	41.099,-0.726,-56.361
	reverse


// Pedestrian number 720

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	32.185,-0.763,-64.995
	point
	31.847,-0.764,-66.235
	reverse


// Pedestrian number 721

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	30.926,-0.748,-70.627
	point
	30.936,-0.755,-72.295
	reverse


// Pedestrian number 722

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	31.045,-0.751,-75.159
	point
	31.379,-0.751,-76.611
	reverse


// Pedestrian number 723

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	32.298,-0.749,-79.374
	point
	32.463,-0.749,-79.867
	reverse


// Pedestrian number 724

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	33.769,-1.401,-88.296
	point
	33.542,-1.511,-89.642
	reverse


// Pedestrian number 725

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	33.000,-1.728,-92.931
	point
	32.566,-1.934,-95.617
	reverse


// Pedestrian number 726

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	32.020,-1.863,-99.275
	point
	31.788,-1.751,-100.886
	reverse


// Pedestrian number 727

10				// Ref num
6				// Number of instructions
5				// Initial instruction

	point
	29.726,-1.023,-106.867
	point
	28.968,-0.997,-107.834
	point
	26.707,-1.253,-110.579
	point
	25.896,-1.317,-111.489
	point
	24.161,-0.903,-113.433
	reverse


// Pedestrian number 728

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	23.541,-0.694,-114.139
	point
	23.209,-0.613,-114.529
	reverse


// Pedestrian number 729

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	20.706,-0.587,-117.867
	point
	20.182,-0.529,-118.412
	reverse


// Pedestrian number 730

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	18.758,-0.284,-119.769
	point
	18.114,-0.176,-120.316
	reverse


// Pedestrian number 731

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	14.410,-0.559,-123.496
	point
	13.097,-0.608,-124.639
	reverse


// Pedestrian number 732

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	14.878,-0.612,-128.312
	point
	15.692,-0.602,-127.727
	reverse


// Pedestrian number 733

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	17.466,-0.422,-126.074
	point
	17.818,-0.330,-125.690
	reverse


// Pedestrian number 734

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	23.175,-0.762,-122.924
	point
	24.412,-0.913,-123.188
	reverse


// Pedestrian number 735

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	26.975,-1.268,-123.550
	point
	28.110,-1.350,-123.632
	reverse


// Pedestrian number 736

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	34.007,-1.618,-122.275
	point
	34.587,-1.646,-122.032
	reverse


// Pedestrian number 737

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	38.986,-1.500,-118.299
	point
	39.412,-1.466,-117.589
	reverse


// Pedestrian number 738

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	41.289,-1.533,-111.598
	point
	41.437,-1.624,-110.440
	reverse


// Pedestrian number 739

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	41.658,-1.726,-106.865
	point
	41.660,-1.724,-106.354
	reverse


// Pedestrian number 740

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	40.583,-1.964,-95.610
	point
	40.493,-1.953,-95.068
	reverse


// Pedestrian number 741

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	39.365,-1.438,-89.523
	point
	38.960,-1.278,-87.647
	reverse


// Pedestrian number 742

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	38.131,-1.044,-83.765
	point
	37.765,-0.929,-82.100
	reverse


// Pedestrian number 743

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	36.378,-0.751,-77.266
	point
	36.274,-0.748,-76.916
	reverse


// Pedestrian number 744

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	35.384,-0.740,-73.844
	point
	35.244,-0.739,-72.475
	reverse


// Pedestrian number 745

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	35.280,-0.749,-68.617
	point
	35.622,-0.749,-66.551
	reverse


// Pedestrian number 746

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	38.744,-0.683,-61.558
	point
	39.152,-0.695,-61.215
	reverse


// Pedestrian number 747

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	33.050,-0.779,-63.015
	point
	32.637,-0.769,-63.772
	reverse


// Pedestrian number 748

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	31.363,-0.758,-68.208
	point
	31.113,-0.751,-69.652
	reverse


// Pedestrian number 749

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	31.146,-0.770,-73.327
	point
	31.187,-0.769,-74.008
	reverse


// Pedestrian number 750

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	32.812,-0.781,-79.383
	point
	32.999,-0.780,-79.966
	reverse


// Pedestrian number 751

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	34.011,-1.206,-86.036
	point
	33.973,-1.230,-86.327
	reverse


// Pedestrian number 752

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	33.311,-1.654,-91.830
	point
	33.226,-1.743,-92.936
	reverse


// Pedestrian number 753

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	31.915,-1.658,-101.796
	point
	31.635,-1.515,-102.903
	reverse


// Pedestrian number 754

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	28.109,-1.050,-109.245
	point
	27.645,-1.132,-110.006
	reverse


// Pedestrian number 755

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	26.738,-1.300,-111.415
	point
	25.819,-1.268,-112.675
	reverse


// Pedestrian number 756

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	24.230,-0.764,-114.583
	point
	24.102,-0.727,-114.700
	reverse


// Pedestrian number 757

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	22.510,-0.554,-116.093
	point
	21.322,-0.583,-117.083
	reverse


// Pedestrian number 758

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	19.356,-0.391,-118.858
	point
	18.445,-0.229,-119.734
	reverse


// Pedestrian number 759

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	13.664,-0.614,-129.365
	point
	12.879,-0.604,-130.160
	reverse


// Pedestrian number 760

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	10.686,-0.581,-132.461
	point
	10.146,-0.523,-133.499
	reverse


// Pedestrian number 761

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	8.431,-0.473,-134.760
	point
	7.975,-0.473,-134.561
	reverse


// Pedestrian number 762

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	7.350,-0.471,-134.255
	point
	6.970,-0.472,-134.005
	reverse


// Pedestrian number 763

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	4.950,-0.369,-134.612
	point
	4.538,-0.367,-135.465
	reverse


// Pedestrian number 764

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	2.689,-0.327,-140.249
	point
	2.429,-0.200,-141.632
	reverse


// Pedestrian number 765

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	2.444,-0.017,-146.202
	point
	2.472,0.097,-147.214
	reverse


// Pedestrian number 766

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	2.620,0.449,-151.761
	point
	2.708,0.647,-153.777
	reverse


// Pedestrian number 767

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	7.459,0.747,-154.591
	point
	7.419,0.697,-153.632
	reverse


// Pedestrian number 768

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	6.922,0.313,-149.786
	point
	6.666,0.167,-148.304
	reverse


// Pedestrian number 769

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	6.664,-0.141,-144.273
	point
	6.656,-0.184,-143.543
	reverse


// Pedestrian number 770

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	7.408,-0.350,-139.912
	point
	7.829,-0.360,-138.985
	reverse


// Pedestrian number 771

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	8.344,-0.361,-137.075
	point
	8.524,-0.365,-136.459
	reverse


// Pedestrian number 772

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	9.352,-0.480,-134.368
	point
	9.827,-0.541,-133.495
	reverse


// Pedestrian number 773

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	10.730,-0.596,-126.904
	point
	11.498,-0.585,-126.037
	reverse


// Pedestrian number 774

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	15.312,-0.361,-122.424
	point
	15.984,-0.204,-121.793
	reverse


// Pedestrian number 775

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	17.027,-0.494,-126.214
	point
	16.384,-0.580,-126.667
	reverse


// Pedestrian number 776

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	7.855,-0.560,-129.520
	point
	7.308,-0.551,-130.140
	reverse


// Pedestrian number 777

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	6.117,-0.495,-131.654
	point
	5.448,-0.453,-132.560
	reverse


// Pedestrian number 778

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	4.629,-0.421,-134.161
	point
	4.132,-0.419,-135.379
	reverse


// Pedestrian number 779

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	3.282,-0.329,-140.153
	point
	3.182,-0.277,-141.260
	reverse


// Pedestrian number 780

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	2.916,-0.135,-144.238
	point
	2.794,-0.046,-145.810
	reverse


// Pedestrian number 781

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	2.751,0.317,-150.515
	point
	2.805,0.407,-151.415
	reverse


// Pedestrian number 782

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	2.890,0.756,-155.433
	point
	2.967,0.781,-156.124
	reverse


// Pedestrian number 783

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	6.794,0.506,-151.699
	point
	6.689,0.373,-150.504
	reverse


// Pedestrian number 784

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	6.929,-0.332,-140.795
	point
	7.151,-0.395,-139.519
	reverse


// Pedestrian number 785

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	25.402,-1.057,-120.805
	point
	26.016,-1.122,-120.861
	reverse


// Pedestrian number 786

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	29.870,-1.428,-120.726
	point
	30.964,-1.503,-120.565
	reverse


// Pedestrian number 787

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	40.126,-1.420,-115.409
	point
	40.484,-1.415,-114.782
	reverse


// Pedestrian number 788

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	41.322,-1.717,-109.029
	point
	41.357,-1.788,-107.555
	reverse


// Pedestrian number 789

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	41.107,-1.697,-102.523
	point
	41.010,-1.713,-101.486
	reverse


// Pedestrian number 790

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	40.073,-1.947,-94.404
	point
	39.501,-1.624,-91.169
	reverse


// Pedestrian number 791

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	38.731,-1.257,-87.197
	point
	38.347,-1.145,-85.358
	reverse


// Pedestrian number 792

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	37.387,-0.893,-81.287
	point
	36.962,-0.773,-79.909
	reverse


// Pedestrian number 793

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	35.850,-0.768,-76.742
	point
	35.323,-0.753,-74.634
	reverse


// Pedestrian number 794

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	34.790,-0.767,-71.456
	point
	35.355,-0.737,-70.175
	reverse


// Pedestrian number 795

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	35.921,-0.735,-68.039
	point
	36.018,-0.733,-66.409
	reverse


// Pedestrian number 796

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	31.619,-0.784,-68.099
	point
	31.378,-0.777,-69.685
	reverse


// Pedestrian number 797

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	32.522,-1.982,-96.769
	point
	32.365,-1.923,-98.653
	reverse


// Pedestrian number 798

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	25.984,-0.872,-116.218
	point
	25.151,-0.663,-116.906
	reverse


// Pedestrian number 799

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	8.244,-0.601,-129.758
	point
	7.495,-0.568,-130.439
	reverse


// Pedestrian number 800

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	4.925,0.850,-163.694
	point
	5.143,0.840,-164.513
	reverse


// Pedestrian number 801

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	6.089,0.728,-167.387
	point
	6.367,0.674,-168.111
	reverse


// Pedestrian number 802

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	8.891,0.402,-168.993
	point
	9.330,0.420,-168.470
	reverse


// Pedestrian number 803

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	9.873,0.670,-166.048
	point
	9.545,0.750,-165.220
	reverse


// Pedestrian number 804

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	8.463,0.807,-162.144
	point
	8.251,0.863,-161.134
	reverse


// Pedestrian number 805

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	7.677,0.834,-158.309
	point
	7.573,0.824,-157.867
	reverse


// Pedestrian number 806

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	3.695,0.848,-159.575
	point
	3.788,0.859,-160.380
	reverse


// Pedestrian number 807

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	4.243,0.874,-162.737
	point
	4.397,0.873,-163.651
	reverse


// Pedestrian number 808

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	4.915,0.850,-165.942
	point
	5.156,0.810,-166.784
	reverse


// Pedestrian number 809

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	6.535,0.510,-169.970
	point
	6.808,0.451,-170.504
	reverse


// Pedestrian number 810

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	11.876,0.334,-177.725
	point
	13.193,0.459,-179.467
	reverse


// Pedestrian number 811

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	14.670,0.657,-181.381
	point
	15.099,0.711,-181.860
	reverse


// Pedestrian number 812

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	16.757,0.760,-182.101
	point
	17.171,0.769,-181.809
	reverse


// Pedestrian number 813

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	17.886,0.777,-181.259
	point
	18.210,0.777,-180.946
	reverse


// Pedestrian number 814

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	18.147,0.685,-178.775
	point
	17.760,0.625,-177.894
	reverse


// Pedestrian number 815

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	15.311,0.313,-174.039
	point
	14.510,0.272,-172.975
	reverse


// Pedestrian number 816

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	12.883,0.258,-170.990
	point
	11.995,0.279,-169.810
	reverse


// Pedestrian number 817

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	9.626,0.438,-168.084
	point
	8.255,0.429,-169.120
	reverse


// Pedestrian number 818

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	7.965,0.353,-170.877
	point
	8.286,0.309,-171.752
	reverse


// Pedestrian number 819

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	9.006,0.266,-173.701
	point
	9.524,0.264,-174.874
	reverse


// Pedestrian number 820

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	12.610,0.369,-178.304
	point
	13.329,0.424,-179.024
	reverse


// Pedestrian number 821

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	14.809,0.605,-180.893
	point
	15.414,0.693,-181.703
	reverse


// Pedestrian number 822

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	18.858,1.072,-187.218
	point
	19.375,1.017,-188.239
	reverse


// Pedestrian number 823

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	25.199,0.744,-194.005
	point
	25.321,0.714,-194.615
	reverse


// Pedestrian number 824

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	25.601,0.393,-201.348
	point
	25.560,0.337,-201.887
	reverse


// Pedestrian number 825

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	25.113,-0.175,-206.408
	point
	24.856,-0.323,-207.816
	reverse


// Pedestrian number 826

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	23.922,-0.501,-210.925
	point
	23.460,-0.506,-212.375
	reverse


// Pedestrian number 827

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	22.030,-0.412,-215.965
	point
	21.788,-0.416,-216.530
	reverse


// Pedestrian number 828

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	20.174,-0.457,-219.304
	point
	19.509,-0.406,-220.316
	reverse


// Pedestrian number 829

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	17.001,-0.131,-223.956
	point
	16.149,-0.078,-225.131
	reverse


// Pedestrian number 830

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	14.601,0.069,-227.257
	point
	13.669,0.205,-228.508
	reverse


// Pedestrian number 831

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	12.749,0.376,-229.591
	point
	12.428,0.440,-229.963
	reverse


// Pedestrian number 832

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	10.459,0.610,-230.543
	point
	10.042,0.615,-230.149
	reverse


// Pedestrian number 833

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	9.607,0.610,-229.598
	point
	9.248,0.606,-229.158
	reverse


// Pedestrian number 834

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	10.029,0.630,-226.896
	point
	10.626,0.630,-226.173
	reverse


// Pedestrian number 835

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	11.171,0.632,-224.909
	point
	10.931,0.630,-223.739
	reverse


// Pedestrian number 836

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	10.403,0.629,-221.642
	point
	10.051,0.628,-219.404
	reverse


// Pedestrian number 837

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	10.006,0.629,-216.844
	point
	10.085,0.630,-215.633
	reverse


// Pedestrian number 838

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	10.263,0.631,-213.982
	point
	10.521,0.630,-212.693
	reverse


// Pedestrian number 839

25				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	11.056,0.630,-210.456
	point
	11.554,0.630,-209.484
	point
	12.784,0.630,-207.458
	point
	13.851,0.630,-206.467
	reverse


// Pedestrian number 840

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	15.638,0.630,-205.224
	point
	16.655,0.631,-204.797
	reverse


// Pedestrian number 841

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	17.956,0.632,-204.628
	point
	18.939,0.631,-204.540
	reverse


// Pedestrian number 842

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	20.202,0.632,-204.031
	point
	20.891,0.631,-203.427
	reverse


// Pedestrian number 843

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	22.066,0.631,-202.250
	point
	22.520,0.632,-201.273
	reverse


// Pedestrian number 844

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	22.434,0.633,-199.784
	point
	22.435,0.626,-199.420
	reverse


// Pedestrian number 845

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	22.954,0.576,-197.155
	point
	23.735,0.582,-196.901
	reverse


// Pedestrian number 846

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	23.563,-0.526,-211.263
	point
	23.361,-0.516,-212.100
	reverse


// Pedestrian number 847

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	21.988,-0.491,-214.083
	point
	21.233,-0.495,-213.785
	reverse


// Pedestrian number 848

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	22.501,-0.456,-214.296
	point
	22.712,-0.468,-213.875
	reverse


// Pedestrian number 849

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	25.304,0.081,-204.256
	point
	25.416,0.173,-203.508
	reverse


// Pedestrian number 850

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	25.647,0.549,-199.350
	point
	25.694,0.587,-198.106
	reverse


// Pedestrian number 851

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	24.282,0.596,-196.496
	point
	24.018,0.586,-196.766
	reverse


// Pedestrian number 852

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	21.714,0.632,-201.552
	point
	21.538,0.632,-201.736
	reverse


// Pedestrian number 853

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	20.217,0.632,-202.894
	point
	19.142,0.631,-203.424
	reverse


// Pedestrian number 854

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	17.779,0.631,-204.108
	point
	17.185,0.632,-204.518
	reverse


// Pedestrian number 855

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	16.027,0.631,-205.481
	point
	15.789,0.631,-205.679
	reverse


// Pedestrian number 856

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	14.022,0.630,-207.167
	point
	13.044,0.629,-208.161
	reverse


// Pedestrian number 857

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	11.010,0.630,-211.288
	point
	10.280,0.631,-212.300
	reverse


// Pedestrian number 858

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	9.737,0.630,-213.710
	point
	9.490,0.630,-214.954
	reverse


// Pedestrian number 859

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	9.657,0.631,-216.413
	point
	9.924,0.630,-217.444
	reverse


// Pedestrian number 860

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	10.554,0.631,-219.403
	point
	10.776,0.631,-220.187
	reverse


// Pedestrian number 861

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	10.993,0.631,-221.555
	point
	11.118,0.630,-222.447
	reverse


// Pedestrian number 862

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	10.782,0.631,-226.415
	point
	10.595,0.631,-227.086
	reverse


// Pedestrian number 863

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	13.217,0.253,-228.809
	point
	13.748,0.175,-228.260
	reverse


// Pedestrian number 864

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	20.650,0.983,-191.728
	point
	20.205,1.017,-190.667
	reverse


// Pedestrian number 865

25				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	18.596,1.093,-187.637
	point
	18.055,1.147,-186.940
	reverse


// Pedestrian number 866

22				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	16.877,1.008,-184.445
	point
	16.614,0.954,-183.992
	reverse


// Pedestrian number 867

18				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	19.857,0.943,-181.180
	point
	20.328,1.025,-181.783
	reverse


// Pedestrian number 868

16				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	23.607,1.023,-188.589
	point
	24.232,0.958,-190.197
	reverse


// Pedestrian number 869

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	21.322,0.861,-193.195
	point
	21.172,0.903,-192.603
	reverse


// Pedestrian number 870

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	20.084,0.988,-189.635
	point
	19.236,1.035,-188.431
	reverse


// Pedestrian number 871

8				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	16.602,0.468,-176.569
	point
	15.529,0.339,-175.136
	reverse


// Pedestrian number 872

7				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	13.445,0.230,-172.236
	point
	12.294,0.241,-170.610
	reverse


// Pedestrian number 873

6				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	9.792,0.230,-173.776
	point
	10.395,0.247,-175.019
	reverse


// Pedestrian number 874

4				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	11.626,0.283,-176.744
	point
	12.309,0.323,-177.617
	reverse


// Pedestrian number 875

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	16.756,0.630,-205.247
	point
	15.570,0.632,-206.161
	reverse


// Pedestrian number 876

2				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	9.951,0.632,-212.299
	point
	9.987,0.630,-214.249
	reverse


// Pedestrian number 877

1				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	9.476,0.673,-226.435
	point
	8.839,0.665,-227.538
	reverse


// Pedestrian number 878

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-140.832,-0.554,-135.541
	reverse


// Pedestrian number 879

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-137.243,-0.827,-133.381
	reverse


// Pedestrian number 880

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-128.902,-0.997,-136.038
	reverse


// Pedestrian number 881

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-117.028,-1.168,-128.207
	reverse


// Pedestrian number 882

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-97.250,-1.000,-128.954
	reverse


// Pedestrian number 883

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-90.476,-1.369,-123.751
	reverse


// Pedestrian number 884

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-74.951,-0.627,-123.387
	reverse


// Pedestrian number 885

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-68.644,-0.972,-124.451
	reverse


// Pedestrian number 886

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-46.895,-1.590,-112.302
	reverse


// Pedestrian number 887

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-41.247,-1.191,-115.898
	reverse


// Pedestrian number 888

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-27.208,-1.160,-110.195
	reverse


// Pedestrian number 889

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-17.581,-0.937,-90.688
	reverse


// Pedestrian number 890

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-27.370,-1.153,-86.039
	reverse


// Pedestrian number 891

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-40.479,-1.220,-88.969
	reverse


// Pedestrian number 892

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-46.338,-0.647,-70.667
	reverse


// Pedestrian number 893

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-52.870,-0.961,-63.333
	reverse


// Pedestrian number 894

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-71.431,-0.550,-59.336
	reverse


// Pedestrian number 895

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.322,-0.785,-62.706
	reverse


// Pedestrian number 896

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-91.352,-0.300,-44.380
	reverse


// Pedestrian number 897

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-97.811,-0.540,-30.497
	reverse


// Pedestrian number 898

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-100.456,-0.711,-5.254
	reverse


// Pedestrian number 899

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-92.902,-0.844,4.045
	reverse


// Pedestrian number 900

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-72.165,-0.652,7.504
	reverse


// Pedestrian number 901

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-75.624,-0.933,23.042
	reverse


// Pedestrian number 902

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.056,-0.577,42.757
	reverse


// Pedestrian number 903

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-97.800,-0.868,45.698
	reverse


// Pedestrian number 904

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-98.770,-0.758,67.733
	reverse


// Pedestrian number 905

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-90.648,-0.575,72.523
	reverse


// Pedestrian number 906

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-78.856,-0.988,79.358
	reverse


// Pedestrian number 907

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-69.605,-1.100,96.046
	reverse


// Pedestrian number 908

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-71.488,-0.704,110.963
	reverse


// Pedestrian number 909

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	44.652,-0.986,144.270
	reverse


// Pedestrian number 910

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	51.435,-0.842,147.708
	reverse


// Pedestrian number 911

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	67.117,-0.714,148.080
	reverse


// Pedestrian number 912

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	73.155,-1.049,143.850
	reverse


// Pedestrian number 913

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	80.623,-1.067,126.090
	reverse


// Pedestrian number 914

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	62.365,-0.712,119.935
	reverse


// Pedestrian number 915

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	62.223,-1.020,111.920
	reverse


// Pedestrian number 916

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	61.003,-0.975,104.524
	reverse


// Pedestrian number 917

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	67.862,-1.149,74.080
	reverse


// Pedestrian number 918

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	68.832,-1.263,51.426
	reverse


// Pedestrian number 919

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	75.814,-1.235,37.944
	reverse


// Pedestrian number 920

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	76.029,-1.235,36.417
	reverse


// Pedestrian number 921

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	69.498,-1.264,19.156
	reverse


// Pedestrian number 922

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	63.262,-1.179,11.002
	reverse


// Pedestrian number 923

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	55.909,-1.047,-7.685
	reverse


// Pedestrian number 924

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	59.669,-0.943,-35.813
	reverse


// Pedestrian number 925

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	56.983,-0.853,-48.725
	reverse


// Pedestrian number 926

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	50.649,-0.818,-50.104
	reverse


// Pedestrian number 927

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.274,-0.772,-66.839
	reverse


// Pedestrian number 928

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.457,-0.776,-75.940
	reverse


// Pedestrian number 929

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	38.196,-1.988,-96.208
	reverse


// Pedestrian number 930

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	39.058,-1.689,-106.261
	reverse


// Pedestrian number 931

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	25.605,-1.112,-123.317
	reverse


// Pedestrian number 932

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.024,-0.601,-127.710
	reverse


// Pedestrian number 933

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	2.757,0.132,-148.145
	reverse


// Pedestrian number 934

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.733,0.837,-159.665
	reverse


// Pedestrian number 935

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.951,1.091,-183.066
	reverse


// Pedestrian number 936

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	21.716,0.669,-199.288
	reverse


// Pedestrian number 937

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	14.564,0.673,-204.817
	reverse


// Pedestrian number 938

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.832,0.676,-216.580
	reverse


// Pedestrian number 939

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	21.591,-0.426,-218.089
	reverse


// Pedestrian number 940

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	16.183,0.830,-182.902
	reverse




START OF OPPONENT PATHS
79                             // Number of path nodes
    -143.973,-0.597,-124.697   // Node #0
    -140.459,-0.652,-133.561   // Node #1
   -133.312,-1.104,-134.820   // Node #2
   -110.554,-1.244,-128.856   // Node #3
   -98.472,-1.076,-127.262   // Node #4
   -78.599,-0.982,-124.582   // Node #5
    -64.809,-1.041,-121.070   // Node #6
    -41.212,-1.112,-114.583   // Node #7
   -20.005,-1.100,-109.808   // Node #8
  -17.283,-1.255,-103.198   // Node #9
   -19.289,-1.290,-91.237  // Node #10
   -27.062,-1.179,-87.552   // Node #11
   -36.402,-1.312,-88.772   // Node #12
   -40.522,-1.292,-87.062   // Node #13
   -45.460,-1.452,-78.272   // Node #14
   -55.345,-0.635,-57.898   // Node #15
   -59.259,-0.921,-57.330   // Node #16
   -66.598,-0.942,-59.744   // Node #17
   -79.255,-0.786,-61.581   // Node #18
   -85.819,-0.590,-59.636   // Node #19
   -89.925,-0.687,-53.839   // Node #20
  -97.335,-0.769,-28.524   // Node #21
    -99.724,-0.476,-17.850   // Node #22
  -101.042,-0.764,-6.298   // Node #23
  -100.174,-0.785,-2.274   // Node #24
  -87.917,-0.438,2.884   // Node #25
  -73.913,-0.721,8.036   // Node #26
  -72.018,-0.868,13.670  // Node #27
  -82.446,-0.679,40.897  // Node #28
  -92.353,-0.632,40.986   // Node #29
  -94.958,-0.790,43.372   // Node #30
  -98.918,-0.170,59.291   // Node #31
  -99.661,-0.724,69.640  // Node #32
  -93.657,-0.444,74.562   // Node #33
  -82.576,-0.954,75.319   // Node #34
  -73.194,-0.923,80.229   // Node #35
  -70.320,-1.103,88.264   // Node #36
  -73.106,-0.663,105.332   // Node #37
  -67.046,-0.982,110.868   // Node #38
  -56.703,-0.601,113.728   // Node #39
   -53.305,-0.691,115.379   // Node #40
   -43.879,-1.682,115.903   // Node #41
    -31.791,-1.041,113.394   // Node #42
   -13.695,-2.115,115.367   // Node #43
   -7.720,-1.749,119.549   // Node #44
   8.804,-1.909,125.036  // Node #45
   25.470,-2.421,133.785  // Node #46
   37.208,-1.040,141.524   // Node #47
   45.852,-0.929,146.171   // Node #48
   54.253,-0.927,145.223  // Node #49
   70.861,-0.827,146.278   // Node #50
   75.447,-0.961,143.034  // Node #51
   78.617,-1.108,128.521   // Node #52
    76.022,-0.821,122.790   // Node #53
    67.837,-0.675,120.429   // Node #54
   62.231,-0.878,116.854   // Node #55
   62.012,-0.984,106.397  // Node #56
   64.001,-0.205,100.378   // Node #57
   65.267,-1.201,75.041   // Node #58
  71.337,-1.273,49.368  // Node #59
  72.167,-1.304,21.979   // Node #60
  60.119,-1.173,5.350   // Node #61
  54.105,-1.092,-4.106  // Node #62
  55.897,-1.036,-18.502  // Node #63
  60.956,-0.981,-37.546   // Node #64
  46.780,-0.809,-54.792  // Node #65
  33.432,-0.808,-66.251  // Node #66
  33.909,-0.824,-78.180 // Node #67
  33.486,-1.993,-98.586   // Node #68
   29.594,-1.069,-109.300   // Node #69
   13.270,-0.666,-127.150   // Node #70
   4.839,0.388,-151.496   // Node #71
   7.769,0.692,-166.151  // Node #72
   19.751,1.072,-185.428  // Node #73
   24.323,0.184,-202.864  // Node #74
   22.050,-0.537,-213.108  // Node #75
   17.086,-0.243,-221.826   // Node #76
   10.986,0.489,-229.579   // Node #77
   7.773,0.757,-232.078   // Node #78
79                                           // Number of path sections
   0,   1,   0, 255,   0, 255,    1.0,    0   // Section #0
   1,   2,   0, 255,   0, 255,    1.0,    0   // Section #1
   2, 3,   0, 255,   0, 255,    0.5,    0   // Section #2
   3,   4,   0, 255,   0, 255,    0.4,    0   // Section #3
   4,   5,   0, 255,   0, 255,    1.0,    0   // Section #4
   5,   6,   0, 255,   0, 255,    1.0,    1   // Section #5
   6,   7,   0, 255,   0, 255,    1.0,    1   // Section #6
   7,   8,   0, 255,   0, 255,    1.0,    1   // Section #7
   8,   9,   0, 255,   0, 255,    1.0,    1   // Section #8
   9,  10,   0, 255,   0, 255,    1.0,    1   // Section #9
  10,  11,   0, 255,   0, 255,    1.0,    1   // Section #10
  11,  12,   0, 255,   0, 255,    1.0,    1   // Section #11
  12,  13,   0, 255,   0, 255,    1.0,    1   // Section #12
  13,  14,   0, 255,   0, 255,    1.0,    1   // Section #13
  14,  15,   0, 255,   0, 255,    1.0,    1   // Section #14
  15,  16,   0, 255,   0, 255,    1.0,    1   // Section #15
  16,  17,   0, 255,   0, 255,    1.0,    0   // Section #16
  17,  18,   0, 255,   0, 255,    1.0,    0   // Section #17
  18,  19,   0, 255,   0, 255,    1.0,    0   // Section #18
  19,  20,   0, 255,   0, 255,    1.0,    1   // Section #19
  20,  21,   0, 255,   0, 255,    1.0,    1   // Section #20
  21,  22,   0, 255,   0, 255,    1.0,    1   // Section #21
  22,  23,   0, 255,   0, 255,    1.0,    1   // Section #22
  23,  24,   0, 255,   0, 255,    1.0,    1   // Section #23
  24,  25,   0, 255,   0, 255,    1.0,    1   // Section #24
  25,  26,   0, 255,   0, 255,    1.0,    1   // Section #25
  26,  27,   0, 255,   0, 255,    1.0,    1   // Section #26
  27,  28,   0, 255,   0, 255,    1.0,    1   // Section #27
  28,  29,   0, 255,   0, 255,    1.0,    1   // Section #28
  29,  30,   0, 255,   0, 255,    1.0,    1   // Section #29
  30,  31,   0, 255,   0, 255,    1.0,    1   // Section #30
  31,  32,   0, 255,   0, 255,    1.0,    1   // Section #31
  32,  33,   0, 255,   0, 255,    1.0,    0   // Section #32
  33,  34,   0, 255,   0, 255,    1.0,    0   // Section #33
  34,  35,   0, 255,   0, 255,    1.0,    0   // Section #34
  35,  36,   0, 255,   0, 255,    1.0,    0   // Section #35
  36, 37,   0, 255,   0, 255,    1.0,    0   // Section #36
  37,  38,   0, 255,   0, 255,    1.0,    1   // Section #37
  38,  39,   0, 255,   0, 255,    1.0,    1   // Section #38
  39,  40,   0, 255,   0, 255,    1.0,    1   // Section #39
  40,   41,   0, 255,   0, 255,    1.0,    1   // Section #40
  41,  42,   0, 255,   0, 255,    0.6,    0   // Section #41
  42,  43,   0, 255,   0, 255,    0.5,    0   // Section #42
  43,  44,   0, 255,   0, 255,    0.7,    0   // Section #43
  44,  45,   0, 255,   0, 255,    0.8,    0   // Section #44
  45,  46,   0, 255,   0, 255,    1.0,    0   // Section #45
  46,  47,   0, 255,   0, 255,    1.0,    0   // Section #46
  47,  48,   0, 255,   0, 255,    1.0,    0   // Section #47
  48,  49,   0, 255,   0, 255,    1.0,    0   // Section #48
  49,  50,   0, 255,   0, 255,    1.0,    0   // Section #49
  50,  51,   0, 255,   0, 255,    1.0,    0   // Section #50
  51,  52,   0, 255,   0, 255,    1.0,    0   // Section #51
  52,  53,   0, 255,   0, 255,    1.0,    0   // Section #52
  53,  54,   0, 255,   0, 255,    1.0,    0   // Section #53
  54,  55,   0, 255,   0, 255,    1.0,    0   // Section #54
  55,  56,   0, 255,   0, 255,    1.0,    0   // Section #55
  56,  57,   0, 255,   0, 255,    1.0,    0   // Section #56
  57,  58,   0, 255,   0, 255,    1.0,    0   // Section #57
  58,  59,   0, 255,   0, 255,    1.0,    0   // Section #58
  59,  60,   0, 255,   0, 255,    1.0,    0   // Section #59
  60,  61,   0, 255,   0, 255,    1.0,    0   // Section #60
  61,  62,   0, 255,   0, 255,    1.0,    0   // Section #61
  62,  63,   0, 255,   0, 255,    1.0,    0   // Section #62
  63,  64,   0, 255,   0, 255,    1.0,    0   // Section #63
  64,  65,   0, 255,   0, 255,    1.0,    0   // Section #64
  65,  66,   0, 255,   0, 255,    1.0,    0   // Section #65
  66,  67,   0, 255,   0, 255,    1.0,    0   // Section #66
  67,  68,   0, 255,   0, 255,    1.0,    0   // Section #67
  68,  69,   0, 255,   0, 255,    1.0,    0   // Section #68
  69,  70,   0, 255,   0, 255,    1.0,    0   // Section #69
  70,  71,   0, 255,   0, 255,    1.0,    0   // Section #70
  71,  72,   0, 255,   0, 255,    1.0,    0   // Section #71
  72,  73,   0, 255,   0, 255,    1.0,    0   // Section #72
  73,  74,   0, 255,   0, 255,    1.0,    0   // Section #73
  74,  75,   0, 255,   0, 255,    1.0,    0   // Section #74
  75,  76,   0, 255,   0, 255,    1.0,    0   // Section #75
  76,  77,   0, 255,   0, 255,    1.0,    0   // Section #76
  77,  78,   0, 255,   0, 255,    1.0,    0   // Section #77
  78,  0,   0, 255,   0, 255,    1.0,    0   // Section #77
0                                                             // Number of cop start points
END OF OPPONENT PATHS
7										// number of material modifiers
// default material
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT								// room for expansion
//	material '0' DIRT ROAD
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT								// room for expansion
//	material '1' SAND
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT								// room for expansion
//	material '2' ROCK'N'GRASS
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT								// room for expansion
//	material '3'ROCK
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT								// room for expansion
//  MATERIAL '4' METAL WITH RIVETS
1.2										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.5										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
0										// sparkiness
3										// room for expansion
MUD1.MAT
//  MATERIAL '5' METAL WITH RIVETS
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
1.5										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT								// room for expansion
// Non CarObjects
3
01TAXI.TXT
02TRASH.TXT
04TRASH.TXT
3									// number of dust shade tables
61, 84, 33								// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"
92, 51, 34								// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"
227, 209, 143							// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"
6								// Number of network start points
-10.172,-0.271,-6.697			//1
0
-3.553,-0.274,-12.028			//2
0
5.447,-0.275,-15.582			//3
90
18.158,-0.270,-24.558			//4
270
14.812,-0.274,-10.135			//5
180
-0.382,-0.271,6.505			//6
180
1										// number of splash files
SPLSHBLU.PIX 								//  name of pixelmapfile for splashes
2
NEWYORK.TXT
